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ABSTRACT


The use of real time parameter estimation methods for dynamic flight modeling in atmospheric turbulence was studied. Real time parameter estimation results of flight data in atmospheric turbulence and in a calm atmosphere were used to explain the problem and identify potential error sources. The use of indirect atmospheric turbulence measurements for real-time parameter estimation in a linear longitudinal dynamics model was studied to account for atmospheric turbulence. It is shown that correcting the measured air data angles makes it possible to account for atmospheric turbulence as a measured explanatory variable in the parameter estimation problem. Commercial off-the-shelf sensors were researched and evaluated, then compared to air data booms. Frequency response of airflow angle vanes, structural response of the air data boom, and the frequency-dependent upwash and time delay were identified and studied as sources of colored noise in the explanatory variables resulting from typical atmospheric turbulence measurement techniques. The theory explaining the frequency dependent upwash and time delay of airflow angle vanes was studied. The resulting upwash and time delay corrections were analyzed and compared to previous time shift dynamic modeling research. Simulation data, as well as flight test data in atmospheric turbulence, were used to verify the upwash and time delay behavior. A methodology was developed to apply real time upwash and time delay corrections to the airflow angle vanes, dramatically improving parameter estimation results over the existing state of the art. Recommendations are given for follow-on theoretical development, flight research, and instrumentation.
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[bookmark: _Toc361522198]CHAPTER I 
Introduction and General Information

This chapter discusses the problem statement, its motivation, a preliminary investigation and its results, hypothesis statement, equations of motion, assumptions, uniqueness of research and its contribution, and finally an outline.
[bookmark: _Toc361522199]Problem Statement
		 
The fundamental problem to be discussed is: given a dynamic system (aircraft) with unknown model parameters flying in atmospheric turbulence, estimate a model of the dynamic system in real time that is simple, non-iterative, accurate in parameter estimates and in parameter error measures, and rapid in its response to changing dynamics. The measurements of this dynamic system are assumed to be noise contaminated by colored noise. Colored noise is defined as non-white noise where white noise data pairs are statistically independent (uncorrelated) and identically distributed (flat power spectrum).
 
The following results are representative of the effect of atmospheric turbulence on aircraft dynamic model parameter estimates. Data were collected using the NASA Langley AirSTAR T-2 subscale generic transport aircraft during low and high atmospheric turbulence conditions. The T-2 aircraft is a 5.5 percent dynamically-scaled generic twin-engine jet transport aircraft. It is outfitted with flight test instrumentation and air data booms with flow vanes on each wingtip. Figure 1 shows a photograph of the aircraft [1, 2]. 





[image: T2_in_flight]
[bookmark: _Ref350252366][bookmark: _Toc361437966][bookmark: _Ref350252454]Figure 1. T-2 subscale jet transport aircraft
Credit: NASA Langley Research Center


Figure 2 shows parameter estimation results from T-2 flight test data using equation-error in the frequency domain and the classical longitudinal aerodynamic model structure in Eq. (1).

						     (1a)	 

		(1b)

Each marker represents a different run, and only the last estimate of each real-time parameter estimation run is shown. The error bars represent or 95.5% confidence bounds. A total of nine runs are represented; six in high turbulence and three in low turbulence. 








T-2 FLT 15 C21 WT04
(High Turbulence)
T-2 FLT 41 C18 WT02
(Low Turbulence)
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[bookmark: _Ref353611627][bookmark: _Toc353222243][bookmark: _Toc361437967]Figure 2. Effect of atmospheric turbulence on T-2 modeling results
(Dr Eugene A. Morelli, personal communication, April 24, 2013 see also Refs.  [48] and [56] )

Figure 2 shows parameter estimation results from T-2 flight test data using equation-error in the frequency domain and the classical longitudinal aerodynamic model structure in Eq. (1).

							     (1a)

		(1b)

Each marker represents a different run, and only the last estimate of each real-time parameter estimation run is shown. The error bars represent or 95.5% confidence bounds. A total of nine runs are represented; six in high turbulence and three in low turbulence. 










Figure 3 shows additional parameter estimation results from T-2 flight test data using equation-error in the frequency domain. 

T-2 FLT 15 C21 WT04
(High Turbulence)
T-2 FLT 41 C18 WT02
(Low Turbulence)


[image: ]     [image: ]   
[image: ]    [image: ]
[bookmark: _Ref354604924][bookmark: _Toc361437968]Figure 3. Additional effects of atmospheric turbulence on T-2 modeling results
 (Dr Eugene A. Morelli, personal communication, April 24, 2013 see also Refs.  [48] and [56] )
)




Determining exactly what characteristic or effect from atmospheric turbulence causes the bias and scatter in the parameter estimation results is an ongoing research topic. It is known that colored noise in the explanatory variables or model outputs causes increased uncertainty and bias [3, 4, 5] in the parameter estimates, similar to what is observed in Figure 2 and Figure 3 during repeated flight test maneuvers in high atmospheric turbulence. It is unknown whether the atmospheric turbulence causes colored noise in the explanatory variables and/or outputs, and if so, what is the source of the colored noise and in which explanatory variables and/or outputs; whether the atmospheric turbulence results in an inadequate model structure, and if so how should the model structure be adjusted; or, if the observed bias and uncertainty in the parameter estimates in atmospheric turbulence are from some other cause.  
[bookmark: _Toc361522200]Motivation

A team comprised of personnel from The University of Tennessee Space Institute (UTSI), Tullahoma, TN, Bihrle Applied Research Inc (BAR), Hampton, VA, NASA Glenn Research Center, Cleveland, OH, and NASA Langley Research Center, Hampton, VA, has successfully developed a prototype Ice Contamination Envelope Protection System (ICEPro) [6, 7, 8, 9].  This work was funded under a grant by NASA’s Research Opportunities in Aeronautics program (ROA-2006), to address the environmental hazard of aircraft icing. In operational flight conditions, an aircraft can encounter atmospheric turbulence and wind shears of varying magnitudes at any time, and many of these atmospheric turbulence encounters can occur in icing clouds.  The ICEPro system facilitates flight envelope protection by making continuous real time stability and control characteristics assessments, which are synthesized into flyable pilot cueing along with visual and aural alerts during in-flight icing conditions. Detection of degraded aircraft stability and control and performance due to icing is carried out by a dynamic inversion control evaluation system (D-ICES) that compares expected aircraft behavior from a prior knowledge base with current measures of those behaviors. When differences reach defined thresholds, real time parameter identification (RTPID) methods are invoked to estimate current stability and control characteristics parameters, which continuously provide envelope protection pilot cueing and alerts.  The development effort included simulation-based design, testing, and verification. A pilot in-the-loop study was conducted to gather pilot performance data and opinions of the utility of ICEPro during simulated icing encounters. Results of the study indicated that the system performed as expected. By effective use of envelope protection cueing on flight displays, pilots were able to mitigate a potentially hazardous icing encounter by avoiding flight conditions and configurations that can result in an upset condition. However, the simulation could not duplicate all of the real-world conditions that could have first-order effects on system performance, such as those due to atmospheric turbulence. 

The remaining technical issues for RTPID and D-ICES methods are their ability to handle atmospheric turbulence. Without an independent measurement of the atmospheric turbulence or some type of atmospheric turbulence model, neither RTPID nor D-ICES (or any other technique) can distinguish between aircraft responses to control inputs and those due to atmospheric disturbances where the frequency content of the atmospheric turbulence is similar to the frequency content of the control inputs or aircraft states.  This recognized deficiency must be resolved in order to provide the flight deck with cueing and information that is neither false, nor ambiguous under all conditions of flight.  
[bookmark: _Toc361522201]Atmospheric Turbulence Sensors
	
Simulation studies accomplished for this work showed that if the atmospheric turbulence could be measured accurately, then real-time parameter estimation developed in previous work [5, 10] could be applied directly to obtain accurate, real-time parameter estimates in atmospheric turbulence, by treating the atmospheric turbulence as a measured input in the aircraft dynamic model. This motivated a search for flight hardware that could accurately measure the atmospheric turbulence.



[bookmark: _Toc361522202]Background


In general, atmospheric turbulence is measured indirectly, because atmospheric turbulence is embedded in the airspeed measurement. The wind velocity vector  relative to the surface of the Earth is found from the vector subtraction: 

					      					        (2)







where  is the true airspeed, and  is the velocity of the aircraft with respect to the Earth, where the Earth is assumed to be an inertial reference. Embedded in the wind velocity vector  are the atmospheric turbulence air velocities. Because  is computed as the difference between two large quantities, it is essential that and  be measured as accurately as possible in order minimize errors in the computed. The most obvious difficulty in measuring atmospheric turbulence using a sensor mounted on an aircraft is removing the aircraft velocity with respect to the Earth. Additional difficulties arise because the aircraft distorts the airflow around it. Once the wind velocity vector is calculated it can be treated as an explanatory variable in the parameter estimation problem. Any inaccuracies in the measurements or calibrations will affect the calculated wind velocity vector and in turn the parameter estimates.  

A number of atmospheric turbulence sensors have been developed over the years. Although successful measurements are possible using a simple 3-axis accelerometer system to determine the response of the aircraft to gusts of wind [11], this can be subject to large errors due to the mass of the aircraft damping the response to atmospheric turbulence. Notess [12] coupled accelerometers with fixed wind vanes and a pitot-static aircraft true air speed (TAS) sensor, whereas Telford and Warner [13] improved on this system with the introduction of a gyro-stabilized platform. Although fixed and rotating vanes [14, 15] have been used to measure airflow relative to the aircraft; it is currently more common to use a differential pressure method [16, 17, 18] to avoid vibration and frequency response problems associated with long air data booms. Further refinement of the hemispherical pressure sensing head used to sense flow angles is described by Wyngaard [19] and Wood [20]. A more advanced instrument is the best aircraft turbulence (BAT) Probe [21, 22, 23] which uses a nine-hole pressure port formation in conjunction with differential global positioning system (GPS) and fast-response accelerometers to give wind vector measurements at 50 Hz. The BAT probe represents the state of the art and its calculated uncertainty is included in Table 1. 

[bookmark: _Ref352617643][bookmark: _Toc356339980]Table 1. BAT probe 1 sigma error
	Parameter
	1 Sigma Error

	
Roll attitude, , (deg)
	0.10

	
Pitch attitude, , (deg)
	0.10

	
Yaw attitude, , (deg)
	0.10

	Angle of Attack, α, (deg)
	0.10

	Angle of Sideslip, β, (deg)
	0.10

	GPS velocity down, VD, (m/s)
	0.01

	GPS velocity north, VN, (m/s)
	0.01

	GPS velocity east, VE, (m/s)
	0.01

	True airspeed, Vt, (m/s)
	0.01




The cutoff 1 sigma error for this work was set at the values of Table 1. Unfortunately, the BAT probe requires extensive calibration and is not sold as a commercial off the shelf unit.
[bookmark: _Toc361522203]Theory




The wind velocity vector is found from the vector subtraction in Eq. (2).  The following matrices are used to transform the true airspeed from the flight path axis  to the earth axis [24, 25, 26]. The multiplication must be performed in the exact order.


                                                (3)

		(4)

The matrix transformation from the flight path axis true airspeed to the earth axis (North, East, and Down) true airspeed is:


                                                                (5)

where

	 = wind speed north

	 = wind speed east

	 = wind speed down

From Eq. (5), the wind velocity components are calculated:

                                                               (6)
Embedded in the wind velocity vector are the atmospheric turbulence air velocities. The effect of atmospheric turbulence during a steady flight condition can be visualized by plotting a time history of the wind vector components and noting the variation in each component as a function of time. 


This theoretical development assumes that the requisite variables in Eq. (6) are measured without error. Practical implementation of this theory necessitates extensive ground and inflight calibrations to account for boom misalignment, upwash, sidewash, angular rate error, boom bending, and response lag characteristics, among others. In typical flight test applications, the Euler attitude angles are measured using an inertial navigation system, while the airflow angles are measured using an air data boom. Any inaccuracies in either measurement system will directly affect the computed wind velocity components. Special emphasis is placed on the word “computed” because the wind velocity components are not directly measured but computed using the vector subtraction in Eq. (6).
[bookmark: _Toc361522204]COTS Sensors

A search was conducted to identify candidate commercial of the shelf (COTS) atmospheric turbulence sensors. Several sensors were identified using state of the art light detection and ranging (LIDAR) [27] technology with an airflow angle accuracy of 1.0 degrees. In comparison, flight test air data booms with traditional air data technology can be calibrated to an accuracy of 0.1 degrees. Unfortunately, the accuracy of LIDAR based sensors requires an order of magnitude improvement to be useful for the present work. Several additional sensors were identified using traditional air data technology [28, 29]. The AIMMS-20 probe by Avantech Research [29] was chosen for further investigation because it provides the most accurate wind determination of all the candidate sensors. The AIMMS-20 probe incorporates state-of-the-art technology including differential GPS and miniaturized components, and makes use of Kalman Filter signal processing algorithms. Table 2 summarizes the AIMMS-20 performance.  

A quantitative comparison between the AIMMS-20 probe and typical flight test air data and inertial instrumentation will yield similar performance specifications for the measurements they have in common. The advantage of the AIMMS-20 probe is that it is packaged as a COTS system. The disadvantage of the AIMMS-20 probe and all of the other COTS products identified is that atmospheric turbulence is not measured directly but computed. Hence, the COTS solutions are no different than applying the theory discussed in Eq. (2-6) to data collected using flight test hardware, such as an air data boom and an inertial navigation system with differential GPS. Furthermore, any errors that affect an air data boom and an inertial navigation system will also affect the COTS atmospheric turbulence sensors. Therefore, it was found that current COTS atmospheric turbulence sensors do not offer a significant advantage over modern flight test hardware.













[bookmark: _Ref350252588][bookmark: _Toc356339981]Table 2. AIMMS-20 probe performance
	Parameter
	1 Sigma Error

	
Longitudinal acceleration, , (g)
	0.003

	
Lateral acceleration, , (g)
	0.003

	
Normal acceleration, , (g)
	0.05

	Angle of Attack, α, (deg)
	0.10

	Angle of Sideslip, β, (deg)
	0.10

	Pitch rate, q, (deg/s)
	0.01

	Roll rate, p, (deg/s)
	0.07

	Yaw rate, r, (deg/s)
	0.01

	Pitch attitude, θ, (deg)
	0.20

	Roll attitude, ϕ, (deg)
	0.20

	Yaw attitude, ψ, (deg)
	0.20

	GPS velocity down, VD, (m/s)
	0.10

	GPS velocity north, VN, (m/s)
	0.10

	GPS velocity east, VE, (m/s)
	0.10

	True airspeed, Vt, (m/s)
	0.20

	Wind velocity down, WD, (m/s)
	0.30

	Wind velocity north, WN, (m/s)
	0.30

	Wind velocity east, WE, (m/s)
	0.30




[bookmark: _Toc361522205]Sources of Colored Noise

Based on the problem statement and the findings from atmospheric turbulence sensors, a search was conducted to identify possible sources of colored noise in the explanatory variables. Possible sources of colored noise in the explanatory variables include: frequency response of airflow angle vanes, frequency response of the boom, wing aerodynamic response to atmospheric turbulence, aerodynamic model structure, pitot-static frequency response, and airframe structural dynamics, among others. 


Several potential sources of colored noise in the explanatory variables were investigated. These included: frequency response of airflow angle vanes, structural response of an air data boom, wing aerodynamic response in atmospheric turbulence, and aerodynamic model structure. The pitot-static frequency response was not investigated because the altitude and airspeed measurements are of secondary effect in aircraft parameter estimation. Altitude and airspeed are used in the non-dimensionalization process but are not primary independent variables in the aerodynamic model Eq. 16 (presented later in this chapter). Also, airframe structural dynamics were not investigated because air data sensors were assumed to be mounted on the nose of the fuselage which was assumed to be relatively stiff compared to wing tip mounted installations. Additionally, since the airflow angles are the explanatory variables with the largest contribution (first term in the Taylor series expansion, Eq. 16) in the dynamic modeling process, the focus will be on the airflow angles. 
[bookmark: _Toc361522206]Hypotheses

1) Colored noise in the airflow angles is a significant source of bias and increased uncertainty in the parameters estimated in atmospheric turbulence. 
2) The classical aerodynamic model structure Eqs. (1) is correct and it should not be modified for aircraft parameter identification in atmospheric turbulence.
[bookmark: _Toc361522207]Equations of Motion

The full nonlinear flat earth 6 degree of freedom (6-DOF) rigid body equations of motion required to model an aircraft in flight consists of a set of 12 non-linear coupled differential equations with constant coefficients [5]. These equations can be classified as the force (7), moment (8), kinematic (9), and navigation equations (10).  The following assumptions are made: The earth is fixed in inertial space, therefore, the aircraft moves with respect to the earth as an inertial reference. However, the aerodynamic forces and moments acting on an airplane depend on the relative motion between the airplane and the atmosphere. Therefore, the forces and moments are related to the aircrafts motion with respect to the atmosphere. Flight in the earth’s atmosphere is close to the earth’s surface and is confined to small distances so that the earth’s surface can be approximated as flat. Gravity is uniform and gravitational forces do not change with altitude.

           (7a)     


  	                   (7b) 	                                 (7c)




	               	      (8a)		                                                           (8b)	                               (8c)
where,

									      (8d)

						      (9a)

								      (9b)



								      (9c)											   (10a)											   (10b)

						    (10c)
Non-dimensional aerodynamic force and moment coefficients for an aircraft can be computed from flight measurements as follows [5]:
Longitudinal:

		(11a)	

		   (11b)

	(11c)
where,

		(11d)

		(11e)
Lateral-Directional:

		(12a)

		(12b)

		(12c)
These expressions retain the full nonlinear dynamics in the equations of motion for a symmetric (x-z plane) rigid aircraft with a fixed mass distribution and constant mass. For local modeling over a short time period, the force and moment coefficients computed from equations (7) and (8)	 can be modeled using linear expansions in the aircraft states and controls: 

	                                                         (13a)

	(13b)

	(13c)

		(14a)

		(14b)

		(14c)




The Δ notation indicates a small perturbation from a reference condition. In each expansion, a single term is shown to represent all relevant and similar control terms, to simplify the expressions. For example, in Eq. (14b), the term  represents all the control terms for, e.g.. In Eq. (14b),  represents the non-dimensional rolling moment at a reference condition, and similarly for the other expansions. 

These coefficients are called the aircraft stability and control derivatives. Each derivative has an aerodynamic explanation. For example, the stability derivative is the change in pitching moment coefficient with varying angle of attack and is commonly referred to as the longitudinal static stability derivative. When the angle of attack of the airframe increases from the equilibrium condition, the increased lift on the horizontal tail causes a negative pitching moment about the center of gravity of the airframe. Simultaneously, the increased lift of the wing causes a positive or negative pitching moment, depending on the fore and aft location of the lift vector, with respect to the center of gravity. These contributions together with the pitching moment contribution of the fuselage are combined to establish the derivative. 

[bookmark: _Toc361522208]Identification Equations


For flight about one flight condition (Altitude and Mach number) the stability and control derivatives are considered as constant model parameters or time invariant, hence the use of the term constant coefficients in describing the governing equations. It is common to separate the problem into two sets of 3 degrees of freedom (3-DOF). One 3-DOF set represents the longitudinal motion, and one 3-DOF set represents the lateral-directional motion. To simplify the problem statement only the 3-DOF longitudinal model is analyzed. This is carried out by setting  in Eqs. (7-10). Further simplification of the longitudinal equations of motion can be achieved using the short period approximation. Most longitudinal flight maneuvers of interest for real time parameter identification purposes occur over relatively short time periods, and therefore involve the short period response. The short period approximation is obtained by assuming that changes in velocity are negligible, and therefore the drag force equation, Eq. (7a), is eliminated.

By setting, assuming that the propulsive forces act through the aircrafts x-axis, and eliminating the drag force equation, the force, moment, and kinematic equations reduce to:

					   (15a)

											   (15b)

						   				   (15c)

The lift and pitching moment coefficients are expressed as the “usual” linear aerodynamic model of the aircraft’s stability and control derivatives.

						   (16a)

		(16b)
This model structure was chosen over that in Eq. (13a and 13c), because the contributions of velocity to lift and pitching moment coefficients are small compared to the other derivatives.

[bookmark: _Toc361522209]Atmospheric Turbulence Model

Turbulence can be considered a cascade of eddies of different sizes or scales.  An ‘eddy’ is a turbulent motion, localized over a region of size l, which is at least moderately coherent over this region. The region occupied by larger eddies also contain smaller eddies. Eddies in the largest size range are characterized by the lengthscale l0 which is comparable to the largest flow length scale L.

The three turbulence scales [30] are the integral length scale (largest), Taylor microscale, and Kolmogorov length scale (smallest). The bulk of the energy is contained in the larger eddies (integral length scale) in the size range lEI = l0/6 < l < 6l0, which is therefore called the energy-containing range. All eddies are unstable and break up, transferring their energy to smaller eddies. These smaller eddies undergo a similar break-up process and transfer their energy to yet smaller eddies, the inertial subrange. This energy cascade – in which energy is transferred to successively smaller and smaller eddies – continues until the Reynolds number is sufficiently small that inertial forces are roughly equal to viscous forces. Molecular viscosity is effective in dissipating at the Kolmogorov length scale (dissipation range). At these small scales, all the kinetic energy of turbulence is converted into heat.

[image: ]
[bookmark: _Toc361437969]Figure 4. Atmospheric Turbulence Length Scales


In comparison to wind tunnel turbulence, the length scales in atmospheric turbulence can be orders of magnitude larger. For example, in wind tunnel turbulence [31], turbulence scales range from microns to 1 meter. In atmospheric turbulence the integral length scale ranges from meters to kilometers. Additionally, atmospheric turbulence is generated in the integral scale and consumes 90% of the atmospheric turbulence lifetime. The transition to the Taylor and Kolmogorov scales represent 10% of the atmospheric turbulence lifetime.

The integral length scale of atmospheric turbulence was implemented in batch simulations and observed in flight data and will be referred as “atmospheric turbulence” in this work. 

Atmospheric turbulence was tested as calm, light, moderate, and severe. Atmospheric turbulence levels were implemented as defined per MIL-F-8785C [32] and were based on a Dryden turbulence spectrum [33]. The atmospheric turbulence velocity components were generated randomly within the guidelines of the Dryden spectrum using individual realizations of random number sequences and added to the aircraft velocity components to generate the total velocity components. This resulted in unique sequences of random numbers for each test.  The three velocity components from the atmospheric turbulence calculations were added to their appropriate body axis velocity components (u, v, and w) calculated from the aircraft dynamic equations.  

						   	(17a)

						   	(17b)

					   	(17c)
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[bookmark: _Ref350252517][bookmark: _Toc361437970]Figure 5. MIL-F-8785c atmospheric turbulence velocities [32]

The root-mean-square turbulent wind speeds are also shown Figure 5 [33] as a function of altitude. According to MIL-F-8785C [32], the probability of exceeding light turbulence levels is between 10-1 and 10-2, for moderate turbulence, the probability is approximately 10-3, and for severe turbulence it is approximately 10-5. Severe atmospheric turbulence levels are rarely encountered, therefore, in this work severe atmospheric turbulence is not considered. 

[bookmark: _Toc361522210]Assumptions and Simplifications

The assumptions and simplifications discussed are collected and repeated for convenience.
1) Sources of scatter and uncertainty in the parameter estimates are assumed to be the result of colored noise in the explanatory variables and/or outputs.
COTS Atmospheric Turbulence Sensors
2) Existing COTS atmospheric turbulence sensors do not offer an accuracy advantage over modern flight test hardware. Additionally, no direct measurement of atmospheric turbulence is currently available. 

Sources of Colored Noise
3) The colored noise investigation was limited to: frequency response of airflow angle vanes, structural response of the air data boom, wing aerodynamic response to atmospheric turbulence, and aerodynamic model structure.
4) The focus is on the airflow angle α, since it is a first order explanatory variable with the largest contribution in the dynamic modeling process. The angle of sideslip β is not considered, because aircraft modeling is restricted to longitudinal motion along its three degrees of freedom.
5) The classical aerodynamic model structure is assumed correct in atmospheric turbulence.

Equations of Motion
6) The aircraft is a rigid body with a fixed mass distribution and has constant mass.
7) The aircraft is symmetrical about the x-z plane.
8) The earth is fixed in inertial space, therefore, the aircraft moves with respect to the earth as an inertial reference. The forces and moments are related to the aircraft’s motion with respect to the atmosphere.
9) Flight in the earth’s atmosphere is close to the earth’s surface and is confined to small distances so that the earth’s surface can be approximated as flat.
10) Gravity is uniform, and gravitational forces do not change with altitude.
11) The aircraft is restricted to longitudinal motion along its three degrees of freedom.
12) The aircraft’s longitudinal aerodynamics is simplified to short period dynamics.

[bookmark: _Toc361522211]Uniqueness of the Research and its Contribution


In this work, the following contributions to the state of the art are established.

1) A major source of colored noise in the explanatory variables for real time parameter identification in atmospheric turbulence is demonstrated and explained. The explanation includes the original derivation first reported in another field of science – airborne wind measurements for atmospheric science – and a detailed unreported derivation.
2) This work demonstrates how to correctly simulate colored noise for longitudinal parameter identification created by atmospheric turbulence on the airflow angle α explanatory variable.
3) It demonstrates that once airflow angle α is corrected, other sensors do not need additional corrections for longitudinal parameter identification. This assumes that accelerations, rates, and attitudes are measured at the center of gravity. This also assumes that the control surface deflections are measured without errors. Both are realistic assumptions in flight test aircraft.
4) It demonstrates that the usual aerodynamic model structure for longitudinal parameter identification is sufficient, and a new model structure is not required.
5) It develops a simple real time methodology that complements the state of the art real time parameter identification method in a steady atmosphe with minimal a priori information.
6) It dramatically improves real time parameter estimation parameters and parameter error measures in atmospheric turbulence over the current state of the art.
[bookmark: _Toc361522212]Outline

The remaining chapters focus on a literature review for real time parameter identification methods with emphasis on frequency domain sequential least squares and an extended Kalman filter (Chapter II), a detailed investigation into the assumed sources of colored noise which includes the frequency response of airflow angle vanes, wing aerodynamic response in atmospheric turbulence, and the structural response of the air data boom (Chapter III), various evaluations of the assumed sources of colored noise using a desktop 3-DOF longitudinal simulation of NASA’s DHC-6 Twin Otter (Chapter IV), an analysis of flight data with light atmospheric turbulence demonstrating the proposed real time methodology and corrections (Chapter V), future studies (Chapter VI), and conclusions (Chapter VII).



[bookmark: _Toc361522213]CHAPTER II 
Literature Review

There are at least two ways to account for atmospheric turbulence in aircraft parameter identification methods, 1) model the atmospheric turbulence mathematically and estimate the corresponding parameters and 2) measure the atmospheric turbulence. In the first approach, the identification of dynamic models containing atmospheric turbulence is classified as a system with state and measurement noise. The three most prevalent methods for identifying dynamic models from flight data are output error, equation error, and filter error. It has been shown that output error and equation error methods yield biased estimates of dynamic model parameters in the presence of atmospheric turbulence [3, 4]. The output error method assumes measurement noise (Gaussian) exists but not state noise (atmospheric turbulence); whereas equation error assumes that state noise exists but not measurement noise. Filter error methods (FEM) represent the most general approach, where the dynamic system model has both state and measurement noise [34]. In the second approach, atmospheric turbulence is measured, treated as a known input, and accounted for in the aerodynamic model structure. This approach can be directly implemented in output error and equation error methods. The approach, however, requires precise measurement of the atmospheric turbulence. Any inaccuracies in the measurements, airflow calibration errors and time delays, angular rates, and accelerations will affect the accuracy of the stability and control derivatives. For these reasons the first approach is more commonly used. If neither approach is used, aircraft responses due to atmospheric turbulence are force-fitted in output error or equation error methods. The force-fit is a result of both methods automatically using other explanatory variables to at least partly explain the effects of atmospheric turbulence. This phenomenon is the source of aircraft parameter identification errors in atmospheric turbulence.

In practice, colored measurement noise (non-Gaussian) is normally seen in flight data due to bias, scale factor, and other systematic errors. In a calm atmosphere, data compatibility methods [35] are designed to remove these systematic errors before the estimation process. In the presence of atmospheric turbulence, no such methods exist. 

The effects of atmospheric turbulence on aircraft measurements are similar to colored noise, in that the frequency content spans the frequency range, with the majority of the power concentrated at lower frequencies on the interval [0.1, 7.0] Hz.  This frequency range overlaps typical aircraft rigid-body dynamic mode frequencies on the interval [0.1, 2.0] Hz. This relationship causes problems in the parameter identification process, because atmospheric turbulence is an unmeasured excitation input in a frequency range that causes significant changes in aircraft dynamics.

Since the non-measurable process noise makes the system stochastic, it requires a suitable state estimator to propagate the states. If filter error methods are used [36, 35, 37, 3, 38], discriminating signal from noise is implemented through weighting matrices that represent assumed measurement and process noise covariance matrices. In this case, adjustment of one or more tuning parameters must be done in simulation. For real-time applications, the required tuning and computational expense of filter error methods makes them difficult to apply in practice. 

The literature review indicates that for non-real-time applications the state of the art for parameter identification in atmospheric turbulence is the FEM proposed by Maine and Iliff [3]. A more detailed explanation is given by Jategaonkar [38]. For real-time applications the state of the art is the Extended Kalman Filter (EKF) implementation proposed by Kashyap [39] and used in the past to estimate aircraft stability and control derivatives [40, 41, 42, 43, 44, 45]. The EKF is an indirect approach which transforms the derivative estimation problem into a nonlinear state estimation problem by artificially defining the unknown derivatives as additional state variables. This enables the EKF to estimate stability and control derivatives, as well as being a suitable state estimator. 
[bookmark: _Toc361522214]Extended system - EKF

In order to demonstrate the required parameter tuning associated with the EFK, one data set will be analyzed from an HFB-320 research aircraft. The Hansa HFB-320 was a forward swept wing business jet operated by the German Aerospace Center (DLR) research institute. This data set and analysis script were available [38, 46] and will be used to determine the lift, drag, and pitching moment stability and control derivatives in atmospheric turbulence. These data are representative of flight tests carried out to excite the longitudinal motion through a multi-step elevator input, resulting in the excitation of the short period dynamic mode and a pulse elevator input resulting in the excitation of the phugoid dynamic mode. The multi-step and subsequent pulse elevator inputs as well as the aircraft response are depicted in Figure 6. The data was sampled at 10 Hz in light atmospheric turbulence. 
[image: ]
[bookmark: _Ref353226165][bookmark: _Toc324245112][bookmark: _Toc361437971]Figure 6. Time history of output and input variables in light atmospheric turbulence [38]


Clear indications of atmospheric turbulence can be seen in Figure 6 during the first five seconds from the time histories and over the complete airspeed, V time history.

Figure 7 represents time histories of the output variables, measured (blue) and estimated (red), and the input variable (elevator deflection) for the HFB-320 aircraft in light atmospheric turbulence. The estimation process was carried out using the extend system EKF with zero process noise (tuning parameters) on the four states (velocity, angle of attack, pitch attitude, and pitch rate) and representative measurement noise. Close inspection reveals a poor match of velocity, angle of attack, and longitudinal acceleration. The poor match is caused by the presence of atmospheric turbulence (process noise).  This is expected because the required tuning parameters that account for the process noise are not employed.
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[bookmark: _Ref354607530][bookmark: _Toc361437972]Figure 7. Time history of output variables (measured & estimated) and input variables [38]
Figures 8, 9, and 10 provide a detailed view of differences between the measured and estimated outputs for the velocity, angle of attack, and longitudinal acceleration with zero process noise. The velocity time history shows significant differences between the measured and estimated output values from 15 seconds to 45 seconds. This is due to atmospheric turbulence and to the pulse elevator input from 25 to 42 seconds. By design, the pulse elevator input excites the phugoid dynamic mode resulting in the velocity variation. The presence of atmospheric turbulence during the velocity variation and the lack of process noise tuning cause the measured and estimated outputs to diverge. Similar patterns are observed for the angle of attack and longitudinal acceleration outputs in Figure 9 and Figure 10, respectively.
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[bookmark: _Ref354608147][bookmark: _Toc361437973]Figure 8. Time history of Velocity, V (m/s) [38]
[image: ]
[bookmark: _Ref353307500][bookmark: _Toc361437974]Figure 9. Time history of Angle of Attack, α (deg) [38]

[image: ]
[bookmark: _Ref353307509][bookmark: _Toc361437975]Figure 10. Time history of Longitudinal Acceleration, ax (m/s2) [38]
The following results (Table 3), averaged over the last 10 estimates, represent the results of applying the extended system EKF with zero process noise to all four state variables. 

[bookmark: _Ref354607764][bookmark: _Toc356339982]Table 3. EKF with zero process noise
	[bookmark: RANGE!A1:D12]Name
	Estimate
	Std. deviation
	Relative Std. deviation (%)

	CD0
	1.96E-01
	9.07E-04
	0.46

	CDV
	-1.16E-01
	8.42E-04
	0.73

	CDα
	8.45E-02
	1.74E-03
	2.06

	CL0
	7.87E-02
	5.67E-03
	7.21

	CLV
	2.11E-02
	5.36E-03
	25.4

	CLα
	4.07E+00
	1.42E-02
	0.35

	Cm0
	7.71E-02
	1.39E-03
	1.80

	CmV
	3.84E-02
	1.32E-03
	3.43

	Cmα
	-9.92E-01
	2.92E-03
	0.29

	Cmq
	1.55E+01
	1.63E-01
	1.05

	Cmδe
	1.17E+00
	3.64E-03
	0.31





Although the time history comparison is poor for several of the outputs shown in Figures 8-10, the stability and control coefficient derivatives and their respective standard deviations are small for all but CLV, the lift velocity derivative. The large deviation in CLV is most likely caused by poor velocity state estimation. This is expected because the lift coefficient variation (sensitivity) with velocity is small in this segment of the airspeed envelope. In aircraft systems identification, a relative standard deviation, of less than 10% is considered excellent. 

In the next example, example 2, the process noise was increased from zero to 0.13 in the velocity state by trial and error. The process noise for angle of attack, pitch attitude, and pitch rate remained zero. Figures 11-13 provide a detailed view of differences between the measured and estimated outputs for the velocity, angle of attack, and longitudinal acceleration.
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[bookmark: _Ref353308465][bookmark: _Toc361437976]Figure 11. Time history of Velocity, V (m/s) [38]

[image: ]
[bookmark: _Toc361437977]Figure 12. Time history of Angle of Attack, α (deg) [38]


[image: ]
[bookmark: _Ref353308482][bookmark: _Toc361437978]Figure 13. Time history of Longitudinal Acceleration, ax (m/s2) [38]


As shown in Figures 11-13 the output matching for velocity, angle of attack, and longitudinal acceleration dramatically improved by adding process noise to the velocity state. However, the improved output matching caused a change in the derivative estimates and deterioration in the relative standard deviations. The following results (Table 4), averaged over the last 10 estimates, represent EKF results with velocity process noise.

[bookmark: _Ref354607861][bookmark: _Toc356339983]Table 4. EKF with velocity process noise
	[bookmark: RANGE!E1:H12]Name
	Estimate
	         Std. deviation
	Relative Std. deviation (%)

	CD0
	1.30E-01
	2.44E-03
	1.88

	CDV
	-7.10E-02
	2.09E-03
	2.95

	CDα
	3.20E-01
	6.04E-03
	1.88

	CL0
	4.66E-02
	6.21E-03
	13.3

	CLV
	3.32E-02
	5.36E-03
	16.2

	CLα
	4.15E+00
	1.97E-02
	0.48

	Cm0
	1.17E-01
	1.86E-03
	1.58

	CmV
	4.27E-03
	1.68E-03
	39.3

	Cmα
	1.02E+00
	3.84E-03
	0.37

	Cmq
	2.94E+01
	3.10E-01
	1.05

	Cmδe
	1.59E+00
	7.65E-03
	0.48




In the next example, example 3, the velocity state process noise remained 0.13, and the angle of attack process noise was increased to 0.1e-004 by trial and error. The process noise for pitch attitude and pitch rate remained zero. Figures 14-16 provide a detailed view of differences between the measured and estimated outputs for the velocity, angle of attack, and longitudinal acceleration.
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[bookmark: _Toc361437979][bookmark: _Toc324245120]Figure 14. Time history of Velocity, V (m/s) [38]
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[bookmark: _Toc361437980][bookmark: _Toc324245121]Figure 15. Time history of Angle of Attack, α (deg) [38]
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[bookmark: _Ref354608158][bookmark: _Toc361437981][bookmark: _Toc324245122]Figure 16. Time history of Longitudinal Acceleration, ax (m/s2) [38]


As shown in Figure 15 and Figure 16, adding process noise to the angle of attack state improved output matching. However, improved output matching caused a change in the derivative estimates and a larger deterioration in the relative standard deviations. The following results (Table 5), averaged over the last 10 estimates, represent extended system EKF results with velocity and angle of attack process noise.








[bookmark: _Ref354607961][bookmark: _Toc356339984]Table 5. EKF with velocity and angle of attack process noise
	[bookmark: RANGE!H15:K26]Name
	Estimates
	Std. deviation
	Relative Std. deviation (%)

	CD0
	1.23E-01
	3.09E-03
	2.52

	CDV
	-6.43E-02
	2.61E-03
	4.05

	CDα
	3.19E-01
	7.42E-03
	2.32

	CL0
	-9.05E-02
	2.00E-02
	22.2

	CLV
	1.48E-01
	1.68E-02
	11.4

	CLα
	4.31E+00
	4.90E-02
	1.14

	Cm0
	1.14E-01
	2.66E-03
	2.33

	CmV
	5.21E-03
	2.34E-03
	44.9

	Cmα
	1.01E+00
	7.91E-03
	0.79

	Cmq
	3.72E+01
	5.39E-01
	1.45

	Cmδe
	1.60E+00
	1.35E-02
	0.84




It was determined by trial and error that adding process noise to the pitch attitude and pitch rate did not improve output matching. In fact, it caused additional changes in the derivative estimates and continued deterioration in the relative standard deviations, results are not shown.

The following table (Table 6) compares the derivative estimates and relative standard deviations (in parenthesis) using the extended system EKF method. In general, there is significant variation in the estimates and deterioration in the relative standard deviations across the three examples.






[bookmark: _Ref354607989][bookmark: _Toc356339985]Table 6. EKF process noise comparison
	
	EKF
Example 1
	EKF
Example 2
	EKF
Example 3

	Name
	Process Noise Zero
	Process Noise Velocity 
	Process Noise Velocity & Angle of Attack

	CD0
	0.1960
	0.1300
	0.1230

	
	(0.46)
	(1.88)
	(2.52)

	CDV
	-0.1160
	-0.0710
	-0.0643

	
	(0.73)
	(2.95)
	(4.05)

	CDα
	0.0845
	0.3200
	0.3190

	
	(2.06)
	(1.88)
	(2.32)

	CL0
	0.0787
	0.0466
	-0.0905

	
	(7.21)
	(13.32)
	(22.16)

	CLV
	0.0211
	0.0332
	0.1480

	
	(25.43)
	(16.16)
	(11.36)

	CLα
	4.0700
	4.1500
	4.3100

	
	(0.35)
	(0.48)
	(1.14)

	Cm0
	0.0771
	0.1170
	0.1140

	
	(1.80)
	(1.58)
	(2.33)

	CmV
	0.0384
	0.0043
	0.0052

	
	(3.43)
	(39.32)
	(44.92)

	Cmα
	-0.9920
	-1.0200
	-1.0100

	
	(0.29)
	(0.37)
	(0.79)

	Cmq
	-15.5000
	-29.4000
	-37.2000

	
	(1.05)
	(1.05)
	(1.45)

	Cmδe
	-1.1700
	-1.5900
	-1.6000

	
	(0.31)
	(0.48)
	(0.84)




In conclusion, it has been shown that extended system EKF results significantly depend on tuning parameters. In other words, the process noise can be turned up on each of the four states to the point that a perfect match is obtained. The good response match may mask discrepancies resulting from unaccounted aerodynamic or other effects, for example aero elastic effects, and as a consequence model improvements may not be obvious. In the worst case, a good response match is obtained when an important parameter has been inadvertently omitted. Therefore, special care must be taken when using this method so that the least amount of process noise is used. 

Additionally, much of the accuracy of the results depends on the measurement noise matrix. How to specify the starting values may not be obvious in each case. Such information may come from laboratory calibration, uncertainty analysis, prior estimation results, or from Fourier smoothing [47]. In general, as the measurement noise values increase the relative standard deviations deteriorate. The same process as depicted in Figure 8 through Figure 16 would replicate this deterioration but for brevity, results are not shown. In the worst case, the measurement noise values are inadvertently low and misrepresent the accuracy of the aerodynamic stability and control derivatives. A brief mathematical explanation of the EKF is provided in the background section.
[bookmark: _Toc361522215]Sequential Least Squares Frequency Domain – RTPID

The combination of the EKF, the difficulty in analytically characterizing the atmospheric turbulence, the inherent nonlinearity of the problem, and the required tuning make the EKF difficult to use in practice. In a steady atmosphere, the state of the art for real-time parameter identification is sequential least squares in the frequency domain proposed by Morelli [10, 5]. This method will be referred to as real-time parameter estimation (RTPID). RTPID uses a recursive Fourier transform to assemble frequency-domain information in real-time, then uses least squares regression, using an equation error formulation, in the frequency domain to compute parameter estimates and error measures. RTPID is simple, non-iterative, and accurate. It provides accurate parameter error measures, is robust to measurement noise, sensor problems (dropouts, time skews, biases, etc.), has a low computation requirement, and rapidly responds to changes in dynamics. 
Recent work by Morelli [48] has studied the use of RTPID in atmospheric turbulence. In that work, the impact of atmospheric turbulence is minimized by increasing the amplitude of the excitation inputs (multi-axis orthogonal optimized multisine inputs) during low atmospheric turbulence and/or sifting the frequency-domain data for each explanatory variable. By sifting out the rigid body dynamics the remaining frequency domain information is discarded.   

Multi-axis orthogonal optimized multisine inputs are effective for stability and control flight testing. The mathematical details of this input design technique can be found in Refs. [5, 49, 50, 51, 52]. These inputs are illustrated in Figure 17 using version 2.0 of System IDentification Programs for AirCraft (SIDPAC) [5, 53] mkmsswp.m function.
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[bookmark: _Ref353491268][bookmark: _Toc361437982]Figure 17. Multiple orthogonal multisine excitation inputs

The general idea is to excite the aircraft using perturbation inputs with frequency content over a range of frequencies that encompass the expected rigid body dynamic modes. The input spectra depicting the orthogonality and desired frequency coverage on the interval [0.1, 2.0] Hz are illustrated in Figure 18.

[image: ]
[bookmark: _Ref353491254][bookmark: _Toc361437983]Figure 18. Multiple orthogonal multisine input spectra


Multi-axis orthogonal optimized multisine inputs require the use of an onboard flight computer. In the work by Morelli [48], the impact of atmospheric turbulence is minimized by increasing the input amplitude. Although effective in light atmospheric turbulence, there are practical limits to this approach. Larger input amplitudes lead to aerodynamic nonlinearities and potentially violent maneuvers.  Because the frequency content of the inputs is known a priori, the predominant dynamic response of the aircraft to the known inputs has a known form in the frequency domain. The idea is to extract or “sift” the portion of the frequency-domain data for each explanatory variable that resulted from the known input. The remaining frequency content is from other sources, such as atmospheric turbulence, modeling errors, and measurement noise, and can be discarded.

The work by Morelli [48] is summarized into several advantages and disadvantages:
Advantages
1) Multi-axis orthogonal optimized multisine inputs maximize the frequency coverage over the desired interval. The inputs are repeatable and easily modified in amplitude, duration, and frequency coverage.
2) The “sifting” process for RTPID in atmospheric turbulence improves the signal to noise ratio (SNR) by sifting the frequencies designed into the multi-axis orthogonal optimized multisine inputs and discarding all other frequency content.
3) Input amplitude is increased to overpower atmospheric turbulence and further increase the SNR. 
Disadvantages
1) Multi-axis orthogonal optimized multisine inputs cannot be flown by a human pilot and require an onboard flight computer.
2) The “sifting” process does not explain the cause of colored noise in the explanatory variables. Additionally, the sifting process calculated better results for simulation data than for flight test data. Several reasons for this result are explained in Ref. [48].
3) Large input amplitudes can lead to: 
a. Violations of aerodynamic model linearity
b. Deviations from planned flight trajectory
c. Discomfort for flight crew and passengers
In this work an analytical technique is developed that accounts for a major source of colored noise in the airflow angle α explanatory variable for real time parameter identification in atmospheric turbulence. In sharp contrast to the extended system EKF and accompanying process noise tuning parameters, process noise (atmospheric turbulence) is accounted for by correcting the airflow angle α measurement.  It will be demonstrated that once the airflow angle α is corrected, other sensors do not need additional corrections. This makes sense since the equations of motion and aerodynamic model structure are derived about the aircraft’s center of gravity. The required sensors for aircraft parameter identification using Eqs. (16) include an air data sensor, attitude sensor, rates and accelerations sensor, and surface position sensor(s). Given the assumption that the aircraft is rigid the attitude, rates, accelerations, and surface position sensors mounted inside the aircraft are not affected by atmospheric turbulence. The air data sensors are by necessity outside of the airframe and are directly affected by atmospheric turbulence. Furthermore, in contrast to the multi-axis orthogonal optimized multisine inputs and the sifting process, classical parameter identification inputs and amplitudes are sufficient. A brief explanation of RTPID is provided in the following section.

[bookmark: _Toc361522216]Real-Time Parameter Identification Background


Because the parameter estimates and parameter error measures from flight test data will be compared between the EKF and RTPID, a brief explanation and references are provided for each method. 
[bookmark: _Toc361522217]Extended System – EKF

The following mathematical summaries follow Jategaonkar [38]. First, the computational details of the linear Kalman filter for state estimation are presented. Second, building on the Kalman filter equations, the computational details of the EKF for state estimation are presented. Third, the computational details of the augmented EKF for both state and aerodynamic stability and control derivative estimation are presented. A detailed derivation of each method is presented in Jategaonkar [38].

Linear Kalman Filter:

A linear stochastic system can be represented by:

							   (18a)

						 		   (18b)

									   (18c)

The addition of process noise causes the system to no longer be deterministic. Therefore it is not possible to integrate the state variables. Rather, it is necessary to incorporate a suitable state estimator. For linear systems, the Kalman filter provides an optimal state estimator [54]. For nonlinear systems, the EKF gives an approximate solution to the problem. 









There are two important assumptions that are made for the processand measurement noise matrices. First, it is assumed that both matrices affect the dynamic system linearly, which allows the additive noise representation in Eqs. (18). Second, the process noise  is assumed to be characterized by a zero-mean Gaussian noise with identity spectral density, and the measurement noise  is assumed to be characterized by a sequence of Gaussian random variables with zero mean and identity covariance. It is further assumed that the process noise and the measurement noise,  and, are uncorrelated and mutually independent. The noise distribution matrices  and  are in general unknown. 
The computational steps of a Kalman filter for linear systems can be summarized as:
Prediction Step (extrapolation/time update)

							     (19)
where,

						     (20)

Correction Step (measurement update)

			     (21)
where,


					     (22)					      

Extended Kalman Filter:

A nonlinear stochastic system can be represented by:


					     (23)


where,  denotes the system parameters appearing in f and g. To apply the computational steps already discussed in the Kalman filter, we need to linearize the nonlinear model. Linear system matrices are defined as:


							     (24)



The elements of the system state and control input matrices, and, are approximated using the central difference formula given by:


			     (25)










where is a column vector with one in the  row and zeros elsewhere, and  and  are small perturbations in each of the  states and  control variables. The matrices  and  are similarly approximated from the observation function. Computational steps of the Extended Kalman filter for nonlinear systems can be summarized as:

Prediction Step (extrapolation/time update)


						    (26)

where,


					    (27)
Correction Step (measurement update)


			    (28)

where,


    (29)
		


Extended System - EKF

In order to estimate aircraft stability and control derivatives (parameters), the parameter estimation problem needs to be transformed into a state estimation problem. This is done by artificially defining the unknown parameters as additional state variables. Here, the system parameter vector  is the output of an auxiliary dynamic system.

											    (30)

An augmented state vector is defined as


									    (31)

The extended system is represented as


						    (32)








where the subscript “a” denotes the augmented variables, and  are system functions of the state and observation equations of the augmented systems, and  is the corresponding process noise matrix. As before, the process noise  and measurement noise  are assumed to be zero mean, uncorrelated and mutually independent;  and  are the corresponding noise distribution matrices.


We can apply the EKF computation procedures to the extended system previously defined to obtain estimates of the augmented states, which contain the unknown system parameters.

Prediction Step (extrapolation/time update)


					    (33)

with initial conditions


								    (34)
and

				    (35)
Correction Step (measurement update)


		     (36)

where


                                     (37)



This formulation of the EKF, together with modeling equations (repeated next for convenience), allows the estimation of the unknown parameter vector   and the states. 

					     (38)

where the lift and pitching moment coefficients are modeled as:


							     (39)

The observation equations are:


									     (40)


where the longitudinal and vertical force coefficients CX and CZ are given by:

								      (41)

The unknown parameter vector Θ, consisting of the stability and control derivatives, is given by:


				   		      (42)

In general, all of the tools used to generate the extended system EKF results are available in a MATLAB software package [38].
[bookmark: _Toc361522218]Sequential Least Squares Frequency Domain – RTPID
		






The real-time parameter estimation algorithm being employed was developed by Morelli [10], and is based on a frequency domain approach implemented in version 2.0 of SIDPAC [5, 53]. A detailed listing of the real-time parameter estimation function rtpid_totter.m is included in APPENDIX 1. The approach uses a linearized model of the vehicle dynamics, where,,andare matrices containing stability and control derivatives, and  and  are the aircraft state and control vectors, respectively:


						     	      (43) 



In Eqs. (43), the stability and control derivatives to be estimated can be dimensional or non-dimensional [5].  Time-varying estimates of the stability and control derivatives are determined using measured aircraft control surface deflections  and measured states  from air flow angle data and angular rate data.   Outputs  are aircraft states and translational accelerations. To determine the model parameter estimates, a cost function is formulated in the frequency domain from the Fourier transform of the model in Eq. (43),

                                                                                                     (44)
The cost function is


  for  frequencies		                   (45)






where  and  are the  row of matricesand, respectively, and.  Each line in Eq. (44) can be analyzed separately in this way, which implements an equation-error formulation [10].  The least squares cost function in each case can be formulated as

							                   (46)
where,


      					                   (47)





and the unknown parameters fromandare contained in the parameter vector . The least squares parameter vector estimate is obtained as the value of  that minimizes the cost function in Eq. (46) [5].

				    	      (48)
Performing the identification in the frequency domain is advantageous for this application because of computational efficiency, robustness to noise and data dropouts, and reliable confidence bounds from the covariance matrix.  This is due to the automatic filtering inherent in using a limited bandwidth for the recursive Chirp Z transform [10], since the rigid-body dynamics of typical piloted aircraft lie in a relatively narrow frequency band of approximately 0.01-2.0 Hz. 


The finite Fourier transform of a signal  is defined by

								     (49)
The corresponding Euler approximation to the integral is defined as

								     (50)
This summation is defined as the discrete Fourier transform,

								     (51)
Therefore, the finite Fourier transformation approximation can be written as

									     (52)
where,

								     	      (53)

The recursive implementation is realized by defining the discrete Fourier transform at any discrete time point 

							      (54)

and defining the discrete Fourier transform at any discrete time point 

									      (55)



For a given frequency, the discrete Fourier transform at sample time  is related to the discrete Fourier transform at time  by

						      (56)



Equation (56) is the recursive Fourier transform. Unfortunately, the frequency spacing is inversely proportional to the number of samples, . A typical (approximately 10 seconds) parameter estimation maneuver will result in coarse frequency spacing. This is exacerbated by the fact that frequency range will span the frequency range up to the Nyquist frequency. A better implementation proposed by Morelli [55] effectively decouples the frequency resolution from the length of the record. This implementation is referred to as the Chirp Z transform. Additionally, the Chirp Z transform allows the user to select a specific frequency band. The recursive Chirp Z transform is implemented by

								      (57)
A detailed derivation of the Chirp Z recursive transform can be found in Morelli [55]. The recursive transforms and calculations in Eq. (14) are done periodically (typically at 1 or 2 Hz) to implement real-time parameter estimation, see Refs. [5] and [10] for details. This RTPID formulation, together with modeling equations (repeated next for convenience), allows the estimation of the unknown parameter vector Θ. 

		  (58a)	

		  (58b)
where,

		 (58c)

		  (58d)


Modeling in the frequency domain can remove biases and trends before the recursive transform calculation. This is effectively accomplished by selecting the frequency vector Hz. This frequency range includes all the rigid-body dynamics in the measured input and output data for the maneuver. Excluding zero frequency effectively minimizes large zero frequency spectral components (associated with trim values and measurement biases) from spilling over and contaminating neighboring frequencies. Additionally, excluding frequencies greater than 2.0 Hz automatically filters wideband measurement noise including structural responses and atmospheric turbulence. 

The lift and pitching moment coefficients are modeled as:

						               (59a)

		   (59b)
The unknown parameter vector Θ consisting of the stability and control derivatives is given by:


							      (60)


[bookmark: _Toc361522219]CHAPTER III
INvestigating sources of colored noise

The effects of the frequency response of airflow angles vanes, the structural response of the air data boom, wing aerodynamic response, and aerodynamic model structure in atmospheric turbulence are investigated as potential sources of colored noise [56]. 
[bookmark: _Toc361522220]Frequency response of airflow angle vanes


IN


In order to investigate the frequency response of airflow angle vanes, a second-order airflow vane sensor dynamic model was studied. A natural frequency of  and a damping ratio of were chosen as representative values for a dynamic model of the airflow vanes [15, 57, 58]. Typical natural frequency and damping ratio values range from 5-20 Hz and 0.2-0.6 respectively. Eq. (61) represents a second order continous-time transfer function for a damped oscillating system:

		 						      (61)

The transfer function representation does not support non-zero initial conditions; therefore, the vane sensor model was converted to a state space representation which supported a trim  initial condition, as defined in MATLAB® tf2ss.m function.
[bookmark: _Toc361522221]Structural response of air data boom

In order to investigate the in-flight structural response of the air data boom, airflow angle flight data collected in a DHC-6 Twin Otter during multiple parameter etstimation maneuvers was analyzed in the frequecy domain using Fourier coefficients [5]. Figure 19 shows the frequency response data for the entire frequency range, up to the Nyquist frequency [59] at 25 Hz. The longitudinal and lateral natural frequencies for the dominant structural modes of the air data boom are approximately 8 and 9 Hz. These natural frequencies are associated with the angle of attack and angle of sideslip measurements, respectively. In Figure 19, the Fourier coeffcients near 8 and 9 Hz are at the noise floor and therefore are not an identifiable error source. Similar results were calculated for  angle of sideslip, but the results are not shown. 

[image: ]
[bookmark: _Ref353612020][bookmark: _Toc361437984][bookmark: _Ref351066160]Figure 19. Fourier coefficients for measured angle of attack


During low-level flight tests over the terrestial and marine boundary layer, a Long EZ research aircraft was used to measure atmospheric turbulence [22]. Details of the aircraft and its instrumentation system are found in the cited reference. The boom motion with respect to the center of gravity (accelerometers installed at each location) is summarized in the following figure [22] (reprinted with permission) during flight in light atmospheric turbulence. The phase trace compares fuselage and probe accelerometer sensors, whereas the magnitude traces represent each individual accelerometer sensor.
[image: C:\Users\bmartos\Documents\PhD UT\PhD Research\Turbulence Probe References\NOAA BAT Probe\tiff\1991-Crawford et al - A Sensitive Fast-Response Probe to Measure Turbulence From Any Airplane_Page_18.tiff]
[bookmark: _Ref353223753][bookmark: _Toc361437985][bookmark: _Ref351066298][bookmark: _Ref317168669][bookmark: _Toc317607692]Figure 20. Comparison between vertical accelerations at the boom and center of gravity [20]


Figure 20 illustrates the complexity of motion for this particular boom-airframe combination. Significant difference is apparent in Figure 20 between the vertical motion of the probe and the center of gravity (CG). Below 0.6 Hz the coherence between the two accelerations is 1.0 with zero phase shift. Between 0.6 Hz and 2.0 Hz the coherence decreases and the phase changes from zero to -45 degrees. Beyond 2 Hz there is no significant relationship between the two accelerations. In other words, in the frequency range of interest for rigid body aircraft dynamics (0.1 to 2.0 Hz), the drop in coherence and phase angle indicates that the angle of attack is different between locations. This in turn results in colored noise in the α regressor. No doubt there would be similarities for other boom-airframe combinations but with different frequency responses. Similar data was not available for the DHC-6 Twin Otter. Therefore, the structural response of the nose boom may be a source of colored noise in the angle of attack regressor but cannot be proven until additional accelerometers (noseboom and center of gravity) are installed and additional flight tests are conducted.  
[bookmark: _Toc361522222]Wing aerodynamic response in atmospheric turbulence

A DHC-6 Series 300M Twin Otter research aircraft was used to study the aerodynamic effects on atmospheric turbulence measurements. Details of the aircraft and its instrumentation system can be found in Ref. [60].  A flush air data system mounted on the nose of the Twin Otter was used as the primary source of air data measurements. Flush air data systems avoid the vibration and frequency response problems associated with long air data booms but require extensive calibrations [61].

It was determined in Ref. [60] that a major flow distortion, which seriously affects the vertical wind velocity measurements near the nose of an aircraft, is the frequency-dependent upwash and time delay. These are shown to be the result of not taking into account the decrease in lift and subsequent decrease in upwash correction with eddy frequency caused by the response of the wing vortex system to atmospheric turbulence, the variation of spanwise loading with eddy frequency, and the longitudinal distance between the angle of attack sensor and the leading edge of the wing, respectively. 

The unsteady aerodynamic analysis in Ref. [60] (derived in detail in APPENDIX 2) was applied to flight data from the NASA Glenn DHC-6 Series 100 Twin Otter aircraft to calculate the angle of attack upwash and time delay as a function of frequency. The required upwash correction and time delay are summarized in Figure 21 and Figure 24, respectively, during flight in light atmopsheric turbulence. Similar results are found in Ref. [60].




[bookmark: _Toc361522223]Upwash as a function of frequency

Figure 21 represents the estimated angle of attack scale upwash correction vs. frequency.


[image: figure7b]
[bookmark: _Ref353226556][bookmark: _Toc361437986][bookmark: _Ref351067085][bookmark: _Ref317169026][bookmark: _Toc317607693]Figure 21. Angle of attack upwash correction versus frequency




The frequency scale is the reduced frequency kb based on the half wing span where  is the angular frequency, b is the wingspan, and U is the true airspeed. The angle of attack upwash correction is explained by examining a sensor model:

	           							      (62)
where,

 = angle of attack bias

 = measured angle of attack

 = true angle of attack

In Figure 21, the vertical axis represents the correction required to calculate the true angle of attack from measured data.


							      	      (63)
At low frequencies (representing flight in a calm atmosphere), the scale factor is approximately 0.75 and increases to 0.90 as kb approaches 2.0. A kb value of 2.0 (using the DHC-6 Twin Otter wing span and 110 knot cruise airspeed) corresponds to approximately 2.0 Hz. Therefore, over the frequency range of interest for rigid body aircraft dynamics (0.1 to 2.0 Hz), the scale factor changes from 0.75 to 0.90 due to atmospheric turbulence. 

The frequency dependant upwash correction is caused by the aircraft’s response to atmospheric turbulence. In Refs. [62, 63] Sears and Von Karman theorized the frequency response of a thin wing (infinite span) to a sinusoidal gust in the direction of flight. The two dimensional Sears function is plotted in Figure 22. For each value of the reduced frequency kc, a vector drawn from the origin to the curve in Figure 22 (top plot) represents the lift in both magnitude and phase. As the reduced frequency kc is increased from zero the magnitude of the lift vector decreases continuously (middle plot). The vector at first lags behind and at approximately kc = 0.6 the vector leads by a progressively greater phase angle (bottom plot). The magnitude and phase angle subplots in Figure 22 are plotted up to kc = 2.0 because this is the frequency range of interest for rigid body dynamics.
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[bookmark: _Ref356252156][bookmark: _Toc361437987]Figure 22. Sears 2-D Function

Flight test data from test points 4, 6, and 7 were selected to verify the changes in lift (magnitude and phase) calculated by the Sears 2-D function. Test point 4 represents flight test data in light atmospheric turbulence without ice. Test points 6 and 7 represents flight test data in a calm atmosphere without ice. Additionally, test points 4, 6, and 7 were chosen because their initial conditions were within 5% of each other (airspeed, thrust setting, and aircraft weight).
[image: ]
[bookmark: _Ref356253500][bookmark: _Toc361437988]Figure 23. Lift force coefficient comparison inside and outside of atmospheric turbulence
 

Figure 23 depicts similar lift force coefficients for test points 6 and 7 (calm atmosphere). As theorized by Sears and Von Karman, test point 4, light atmospheric turbulence without icing, shows a decrease in lift coefficient throughout its time history as compared to the calm atmosphere test points. The phase differences cannot be inferred in Figure 23 because piloted inputs were applied at different times.

In Ref. [60] , the changes in lift calculated by the Sears 2-D function SG are linked to a calm atmosphere upwash model.

								      (64)

where,

 = Sears 2-D function

 = lift curve slope

 = lift efficiency term

 = distance between sensor and the wings aerodynamic center

 = upwash angle

Equation 64 relates the changes in lift (Sears 2-D function) to the upwash angle and in turn to the angle of attack (Eq. 63). Therefore, as the lift decreases with reduced frequency the upwash correction approaches unity (Figure 21). 
[bookmark: _Toc361522224]Time delay as a function of frequency

Figure 24 depicts the time delay as a function of frequency. The time delay is primarily caused by the separation between the nose boom mounted airflow vanes (measurement position) and the aircraft’s center of gravity.

[image: figure6b]
[bookmark: _Ref353226569][bookmark: _Toc361437989][bookmark: _Ref351067055]Figure 24. Time delay versus frequency


The magnitude of the time delay represents the correction required to calculate the true angle of attack from measured data. In the frequency range of interest for rigid body aircraft dynamics (0.1 to 2.0 Hz), the time delay is approximately 0.1 seconds. 

Data compatibility [5] analysis was used to reconstruct the angle of attack from inertial flight test measurements and compare that to the measured angle of attack. Three runs were evaluated at similar airspeeds (120 knots) and aircraft configurations. The first run represents a calm atmosphere; the next two runs represent atmospheric turbulence.
[image: TimeDelayComparison_3_runs]
[bookmark: _Ref353612721][bookmark: _Toc361437990][bookmark: _Ref351067669]Figure 25. Angle of attack time delay in atmospheric turbulence


In Figure 25, run 1 in calm atmospheric conditions shows a time delay of approximately 0.03 seconds. Runs 2 and 3 in atmospheric turbulence show a time delay of approximately 0.13 seconds. This agrees with the fact that the time it takes to travel 21 feet (longitudinal distance from the airflow angle measurement position to the center of gravity) at 120 knots is approximately 0.1 seconds. The difference is attributed to forced (elevator doublets) oscillations in run 1 and a combination of forced and atmospheric turbulence oscillations in runs 2 and 3. This increase in time delay in atmospheric turbulence is a source of degradation in the stability and control parameter estimates. Another problem with using inertial measurements to reconstruct data such as angle of attack is that the reconstruction assumes the atmosphere is fixed relative to the earth axes. When there are gusts or winds, this assumption is not valid, and the reconstructed data have errors. Since the airflow angles are measured at the nose of the aircraft and the inertial measurements are taken at the center of gravity, it is expected that the measured angle of attack will lead the reconstructed inertial angle of attack. However, the reconstructed angle of attack leads the measured angle of attack and is in error in Figure 25. This is attributed to not accounting for gusts and winds in the data compatibility analysis.
[bookmark: _Toc361522225]Aerodynamic model structure



It is conceivable that the aerodynamic model structure is different in atmospheric turbulence than in smooth air, although such differences have not been documented in flight [64]. An alternative aerodynamic model structure to Eqs. (16) includes two new stability derivatives and. These parameters represent the non-dimensional pitching moment due to αs (rigid body dynamics) and the non-dimensional pitching moment due to αG (atmospheric turbulence) respectively.  Similar coefficients were implemented for the normal force. The aerodynamic model structure in Eqs. (16) is converted to the body axis for convenience.


	 					   (16a)

						   (16b)





The new stability derivatives and represent different contributions due to the effect of atmospheric turbulence on the aircraft. Stated differently, knowing the effect of atmospheric turbulence on α sensor does not imply that the effect of atmospheric turbulence on the aircraft response can be calculated by simply multiplying α by the usual α stability derivatives, and. It is assumed that the effect of atmospheric turbulence on aircraft response is proportional to the effect of atmospheric turbulence on the α sensor; therefore, atmospheric turbulence coefficients are estimated using turbulent α as a regressor to capture its effect. So it’s not really a turbulent α coefficient as much as it is an effect of atmospheric turbulence using the best measure of atmospheric turbulence. 
Alternate atmospheric turbulence aerodynamic model structure:


					   (65a)

				   (65b)

Simulated test results of this model are presented in the next chapter. In summary, this chapter investigated the frequency response of airflow angles vanes, the structural response of the air data boom, wing aerodynamic response, and aerodynamic model structure in atmospheric turbulence as potential sources of colored noise. An airflow vane dynamic model was proposed to investigate (via simulation) contributions to colored noise. Frequency based airflow angle α calculations showed that the air data boom was insensitive to vibrations but additional testing was recommended. It was determined that a major flow distortion, which seriously affects the vertical wind velocity measurements near the nose of an aircraft, is the frequency-dependent upwash and time delay. Lastly, an alternative aerodynamic model structure was suggested with additional atmospheric turbulence coefficients.


[bookmark: _Toc361522226]CHAPTER IV 
Simulated test results

The effects of the frequency response of airflow angles vanes and the wing aerodynamic response in atmospheric turbulence are investigated as potential sources of colored noise. Results are generated from batch simulations of the DHC-6 Series 100 Twin Otter described in Chapter I and compared against baseline runs with perfect angle of attack measurements.
[bookmark: _Toc361522227]Simulation Test Cases

The hypothesis was tested using a simulation of the DHC-6 Series 100 Twin Otter and the following test conditions:
1) Baseline runs with perfect angle of attack measurements
2) Runs with a representative frequency response model for the airflow angle vanes
3) Repeat test condition 2) with varying angle of attack magnitude and time delay as a function of frequency


4) Runs with additional atmospheric turbulence stability derivatives andand perfect α measurements.
The following parameters are common to all four test conditions:
- Aircraft trimmed at 2,500 feet and 110 knots
- 20 second runs
- Real-time parameter estimation method [3, 8], described in Chapter III
- Orthogonal multi-sine inputs [5] invoked from 1 to 11 seconds
- Model parameter estimates taken at the end of each 20-second run
- 200 runs per atmospheric turbulence intensity (calm, light, moderate, and severe)
- Fourier transform frequency range [0.1 2.0] Hz
- Fourier transform frequency spacing 0.04 Hz
- Signal to noise ratio of 50
- 50 Hz data rate
The following comments are common to all of the figures associated with test conditions one through three:
- Green line = truth value of the parameter
- Red dashed line = confidence interval using ±10% of truth value of the parameter
- Red diamond = parameter estimate
- Blue bars = estimated two sigma error bounds (95.5% confidence bounds)

In the dynamic modeling process, no attempt was made to estimate the axial force coefficients, because the aircraft excitations did not appreciably change airspeed, resulting in a low signal-to-noise ratio for the axial force coefficient parameter estimation. In total, six model parameters were estimated,  
[bookmark: _Toc361522228]Noise for Simulated Time Histories

Gaussian measurement noise was added to the regressors using the SIDPAC buzz.m function. The signal to noise ratio was set at 50. This is typical of flight test instrumentation systems. Atmospheric turbulence (process noise) was tested as calm, light, moderate, and severe. Atmospheric turbulence implementation and levels were defined per MIL-F-8785C [32] and were based on the Dryden turbulence spectrum [33]. The turbulence velocity components were generated randomly within the guidelines of the Dryden spectrum and added to the aircraft velocity components to generate the total velocity components as defined in Chapter I. A random number was used to generate the velocity components from the turbulence spectrum.  Using a varying random number seed results in unique sequences of random numbers from test to test.  The three velocity components from atmospheric turbulence calculations were added to their appropriate wind frame velocity components (u, v, w) that were generated from the aircraft dynamics so that the velocity components used for the vehicle motion calculations included the components from the atmospheric turbulence model.
[bookmark: _Toc361522229]Simulated Data with Noise from Air Data Boom Flexure


As shown in Figure 26, the baseline model estimates for resulted in improved estimates with increasing atmospheric turbulence. This is not representative of actual flight data and is attributed to perfect α measurement given the additional excitation caused by atmospheric turbulence.

[image: Perfect_Sensor_2Hz_df04_no_kb_no_delay_Page_08]

[bookmark: _Ref353225283][bookmark: _Toc361437991][bookmark: _Ref317171316][bookmark: _Toc317607695]Figure 26. Test condition 1 - effect on 




As shown in Figure 27, the baseline model estimates for resulted in greater scatter as turbulence intensity increased. This is caused by noisy explanatory variables [65] from the atmospheric turbulence implementation in Eq. (17).  Similar patterns were observed with the remaining coefficients, results are not shown. These simulations demonstrate that if the angle of attack measurements are perfect, all model parameters can be estimated accurately for any level of turbulence.  
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[bookmark: _Ref353225351][bookmark: _Toc361437992][bookmark: _Ref317171390][bookmark: _Toc317607696]Figure 27. Test condition 1 - effect on 
[bookmark: _Toc361522230]
Simulated Data with Noise from Airflow Vane Dynamics



Estimates for  using the second-order vane sensor model of Eq. (61)                              () caused degradations and biasing in the estimates with increasing atmospheric  turbulence intensities, as shown in Figure 28. This is representative of actual flight data. 
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[bookmark: _Ref353225453][bookmark: _Toc361437993][bookmark: _Toc317607697]Figure 28. Test condition 2 - effect on 




As shown in Figure 29, the baseline model estimates for resulted in greater scatter as atmospheric turbulence intensity increased. This is caused by noisy explanatory variables [65] from the atmospheric turbulence implementation in Eq. (17), and the vane sensor model. Similar patterns were observed in the remaining coefficients
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[bookmark: _Ref353225492][bookmark: _Toc361437994][bookmark: _Ref317171528][bookmark: _Toc317607698]Figure 29. Test condition 2 - effect on 






[bookmark: _Toc361522231]Augmented Simulated Data with Noise from Airflow Vane Dynamics

Although no quantitative analysis was done, qualitatively, small differences were observed between a perfect and a representative airflow vane frequency response in test conditions 1 and 2. The vane dynamics do not substantially contribute to the scatter in the estimates, because all of the added dynamics are outside the range of frequencies analyzed.




To further validate this claim, additional testing was carried out using the same simulation. A total of 121 different combinations of airflow angle vane natural frequency and damping ratios were tested. The natural frequency values tested were 5 through 15 Hz in 1 Hz increments. The damping ratio values tested were 0.01, 0.05, 0.1, 0.15, 0.2, 0.25, 0.3, 0.35, 0.4, 0.45, and 0.6. Since the AIMMS-20 probe approaches a gain of one and zero phase shift, it is characterized by the results of test condition 1. The AIMMS-20 probe offers superior frequency response performance to mechanical vanes by using 1) a 5 hole pressure probe , 2) short tube lengths (air data tubes are typically less than 5 inches long), and 3) the resonance frequency of the silicon pressure diaphragm is in the kilohertz region. The following figures depict the results of 121 combinations, times 4 atmospheric turbulence levels, times 200 runs per case. This totaled 96,800 runs. Figure 29 depicts the results of 96,800 runs for. As an example, the bottom left corner block in severe atmospheric turbulence is light blue. The color represents the number of exceedances of  from ±10% of truth. The remaining 120 blocks are dark blue representing less than 10 exceedances. Figure 30 suggests that any combination of natural frequency and damping ratio tested provides adequate performance. Similar results were obtained for results are not shown. 
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[bookmark: _Ref353225595][bookmark: _Toc361437995][bookmark: _Toc317607699]Figure 30. Number of exceedances for














Figure 31 shows that independent of the natural frequency and damping ratio tested, accurate estimates of  are not feasible in atmospheric turbulence (greater than 60 exceedances) for all atmospheric turbulence levels. This is expected since the model parameter for normal force produced by elevator deflection, , is an order of magnitude less than the model parameter for normal force produced by angle of attack, . This means the signal-to-noise ratio for parameter estimation is an order of magnitude lower for  compared to. 
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[bookmark: _Ref353225759][bookmark: _Toc361437996]Figure 31. Number of exceedances for 

Figure 32 shows that, independent of the natural frequency and damping ratio tested, accurate estimates of  are feasible in atmospheric turbulence. This is expected due to strong elevator control authority.
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[bookmark: _Ref353225797][bookmark: _Toc361437997]Figure 32. Number of exceedances for 


Results for , not shown, demonstrate that independent of the natural frequency and damping ratio tested, exceedances less than 20 out of 200 are not feasible in any level of atmospheric turbulence except calm. For the remaining stability and control estimates, the results show that most combinations of natural frequency and damping ratio tested provide adequate performance in calm, light, moderate turbulence, and severe atmospheric turbulence.
[bookmark: _Toc361522232]Simulated Data with Noise from Wing Response


As shown in Figure 33, estimates for resulted in degraded estimates with increasing atmospheric turbulence for varying angle of attack magnitude and time delay as a function of frequency implemented using the data in Figure 21 and Figure 24. The degradation is seen as biasing in the estimates and increased scatter and uncertainty estimates. This is representative of actual flight data.
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[bookmark: _Ref353225844][bookmark: _Toc361437998]Figure 33. Test condition 3 - effect on 


As shown in Figure 34, the estimates for  also resulted in degraded estimates with increasing atmospheric turbulence. The degradation is seen as biasing in the estimates and increased scatter and uncertainty estimates. The increase in biasing and uncertainty compared to estimates is caused by the relatively small contribution of the elevator term to the normal force coefficient. 
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[bookmark: _Ref353225868][bookmark: _Toc361437999]Figure 34. Test condition 3 - effect on 



Figure 35 shows that the estimates for  degraded with increasing atmospheric turbulence. The degradation is seen as biasing in the estimates and increased scatter and uncertainty estimates. This is representative of actual flight data.
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[bookmark: _Ref353225900][bookmark: _Toc361438000]Figure 35. Test condition 3 - effect on 




As shown in Figure 36, the estimates for  degrade with increasing atmospheric turbulence. The degradation is seen as biasing in the estimates and increased scatter and uncertainty. The estimates for  resulted in the largest biasing of all the aerodynamic estimates considered because angular velocity model parameters are most susceptible to time delays [66]. 
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[bookmark: _Ref353225924][bookmark: _Toc361438001]Figure 36. Test condition 3 - effect on 



Figure 37 shows that the estimates for  degrade with increasing atmospheric turbulence. The degradation is seen as increased scatter and uncertainty in the estimates. This is representative of actual flight data and correlates with the flight results presented in Figure 2 and Figure 3.
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[bookmark: _Ref353225949][bookmark: _Toc361438002]Figure 37. Test condition 3 - effect on 







Corrupting the angle of attack measurement by a frequency-dependent magnitude and time delay affected all of the estimated stability and control coefficients. The estimates of  and  exhibited moderate biasing and increased scatter and uncertainty,  and  estimates had large biases and increased scatter and uncertainty, and  estimates showed the largest biases and increases in scatter and uncertainty. Previous work on the effects of time-shifted data on flight determined stability and control estimates [66] using the output-error method in the time domain demonstrated similar trends in biasing and increased uncertainty, compared to the results shown here due to atmospheric turbulence.
[bookmark: _Toc361522233]Simulated Data for Aerodynamic Model Structure Investigation






Additional atmospheric turbulence stability derivatives and were added to the classical aerodynamic model structure in Eqs. (16). All of the parameter identification estimates for except for the estimates in calm atmosphere resulted in large degradations. In fact, the degradations were so large that they were not captured by the standard plot range used in Figure 26 through Figure 29 and Figure 33 through Figure 36. A similar pattern was observed with the estimates of. This is not representative of actual flight data as shown in Figure 2 and Figure 3 and described in the problem statement. Similar patterns were observed with the remaining coefficients, results are not shown. These results and the three previous simulation cases suggest that the classical aerodynamic model structure in Eqs. (16) is correct and that model structure is not a major source of colored noise.

In summary, this chapter investigated the effects of the frequency response of airflow angles vanes and the wing aerodynamic response in atmospheric turbulence as potential sources of colored noise. It was determined that vane dynamics do not substantially contribute to the scatter in the estimates, because all of the added dynamics are outside the range of frequencies analyzed. Corrupting the angle of attack by a frequency dependent magnitude and time delay corrupted the stability and control derivatives as shown in the problem statement (Figure 2 and Figure 3). Additionally, it was shown that the classical aerodynamic model structure was not a major source of colored noise. 
[bookmark: _Toc361522234]
CHAPTER V 
[bookmark: _Toc361522235]Analysis of flight data in atmospheric turbulence


The airflow angle α, frequency-dependent upwash, and time delay have been identified as significant contributors to biasing and increased uncertainty in parameter identification during atmospheric turbulence. This represents a significant find and advances the state of the art. This chapter develops a real-time methodology to correct airflow angle α measurements resulting in calm air estimates in atmospheric turbulence. Three examples in light atmospheric turbulence were analyzed. First, a longitudinal doublet input during light atmospheric turbulence without icing. Second, a longitudinal doublet input during a calm atmosphere and then entering light atmospheric turbulence without icing. Third, a longitudinal doublet input during light atmospheric turbulence with icing.


Flight test data was gathered during the 2001 Smart Icing System (SIS) flight number 010302f1 [67]. The data record is approximately 2.5 hours at 50 Hz data rate. The data record was inspected for atmospheric turbulence using a modified version of the procedure suggested by Morelli [48]. In that work, the power spectral density of the vertical component of airspeed was calculated in real-time using a sliding data window. Similarly, in the computation of the standard deviation for this work, only the power in the 2 Hz to 7 Hz range was used. Frequencies bellow 2 Hz were associated with flight test inputs. Frequencies above 7 Hz were associated with structural dynamics. The resulting standard deviation in the 2 Hz to 7 Hz range was assumed to exist due to atmospheric turbulence. In that work, atmospheric turbulence levels were determined through comparisons to subjective atmospheric turbulence pilot ratings. In this work, atmospheric turbulence levels were quantified using the Twin Otter simulation (Chapter II) and MIL-F-8785C definitions for light and moderate atmospheric turbulence. The MIL-F-8785C definitions are internationally accepted. Figure 38 and Figure 39 quantify light and moderate atmospheric turbulence for the Twin Otter aircraft.
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[bookmark: _Ref354432009][bookmark: _Toc361438003]Figure 38 Twin Otter Simulation with Light Atmospheric Turbulence
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[bookmark: _Ref354432024][bookmark: _Toc361438004]Figure 39 Twin Otter Simulation with Moderate Atmospheric Turbulence
In Figure 40, the top plot represents the vertical velocity, w, in feet per second. The middle plot represents the vertical velocity standard deviation from 2 Hz to 7 Hz range. The bottom plot represents longitudinal input (doublet) markers recorded by a flight test engineer. The intensity scale in Figure 40 matches Figure 38 (light atmospheric turbulence). Therefore, all atmospheric turbulence in flight 010302f1 is classified as light atmospheric turbulence. This is expected since MIL-F-8785C [32] defines the probability of exceeding light atmospheric turbulence is between 10-1 and 10-2, for moderate atmospheric turbulence, the probability is approximately 10-3, and for severe atmospheric turbulence it is approximately 10-5. Therefore, moderate and severe atmospheric turbulence levels are rarely encountered.  
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[bookmark: _Ref354432190][bookmark: _Toc361438005]Figure 40   and doublet markers plots

Test points 1 through 12 are marked by red vertical lines (from left to right) in Figure 40 and represent the following conditions:

TEST POINT 1 – No ice in light atmospheric turbulence (data was corrupt and unusable)

TEST POINTS 2 – 3 All surfaces iced in light atmospheric turbulence

TEST POINT 4 – All surfaces de-iced in light atmospheric turbulence

TEST POINT 5 – All surfaces iced in calm atmosphere

TEST POINT 6 - Wings de-iced in calm atmosphere

TEST POINT 7 – Horizontal tail de-iced in calm atmosphere

TEST POINT 8 – Vertical tail and struts de-iced in calm atmosphere

TEST POINTS 9 – 11 All surfaces iced in light atmospheric turbulence

TEST POINT 12 – All surfaces de-iced in light atmospheric turbulence

An ideal baseline represents flight data without ice and without atmospheric turbulence. Unfortunately, the data record did not include such representative data. Test points 6-8 represent the best case baseline data.  Test point 6 represents a de-iced wing in calm atmosphere. Test point 7 represents a de-iced wing and horizontal tail in calm atmosphere. Test point 8 represents a de-iced wing, horizontal tail, vertical tail, and struts in calm atmosphere. Test points 6-8 were analyzed and used as baseline data. In addition, three test points in light atmospheric turbulence were analyzed: Test point 4 represents all surfaces de-iced in light atmospheric turbulence (represents the greatest atmospheric turbulence without ice), Test point 2 represents all surfaces iced in light atmospheric turbulence (represents the greatest icing accumulation in atmospheric turbulence), and Test point 12 represents all surfaces de-iced in light atmospheric turbulence (represents a case where  parameter identification inputs were applied in a calm atmosphere, and the aircraft subsequently experienced light atmospheric turbulence).

[bookmark: _Toc361522236]Identification from flight data in light atmospheric turbulence

[image: ]
[bookmark: _Ref355034509][bookmark: _Toc361438006]Figure 41. Test point 4 input and output flight data


Figure 41 plots the longitudinal input and outputs during test point 4 in light atmospheric turbulence without icing.  The angle of attack (α) and normal acceleration (az) time histories show traces of atmospheric turbulence throughout the data run. The longitudinal input () is representative of a doublet input. A doublet is characterized by evenly spaced pulses of equal magnitude in both directions (stick forward and stick aft) starting and returning to a trim condition. The non-square peaks are representative of real flight control systems were the pilot is unable to move the controls at an infinite rate without overshoot. During test point 4, the aircraft’s angle of attack response to a doublet was greater than the response caused by atmospheric turbulence. During the doublet input the aircraft experienced ± 0.25 g’s from a 1 g reference condition.


Figure 42 depicts longitudinal parameter identification estimates for test point 4 using six different methods. Each method is labeled in Figure 42 with callout numberings 1) through 6), respectively.  Test points 6-8 are plotted as a baseline reference with green markers. Two sigma error bars (95.5%) are plotted for each estimate; however, for test points 6-8 the error bars are smaller than the estimate markers. The parameter estimates and two sigma error bars for all methods are included in APPENDIX 4. The following section describes each method and compares its results with the state of the art. The state of the art is method 6, extended system EKF, described in Chapter II. 






It is common practice to omit  from the parameter identification results because these stability and control coefficients are typically an order of magnitude less than. However, in this analysis both  are included. Additionally in Chapter IV, the stability and control coefficients were modeled in the body axis, i.e., instead of the wind axis. In this analysis, modeling was done in the wind axis. Modeling in the wind axis is more difficult than in the body axis because body axis forces must be transformed to the wind axis by the airflow angle. This transformation adds noise and uncertainty to the estimation process.
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[bookmark: _Ref354432442][bookmark: _Toc361438007]Figure 42. Test point 4 Light Atmospheric Turbulence without Icing
[bookmark: _Toc361522237]Description and analysis of methods in light atmospheric turbulence

There are six parameter identification methods used to analyze Twin Otter flight data in light atmospheric turbulence. Method I, equation error in the time domain, is derived in detail in Refs. [67, 5]. Methods II through V are based on RTPID described in Chapter II. Method 6 is the extended system EKF described in Chapter II. Where appropriate, derivations and computational details are provided to reproduce the results. 
[bookmark: _Toc361522238]Method I

Method I represents parameter identification results using equation error in the time domain [67, 5] and SIDPAC lesq.m function. Twin Otter flight data provided by NASA includes sensor corrections for all parameter identification measurements. This includes airspeed position error corrections, airflow angle alignment and position errors, and accelerometer position errors among others. 
The parameter identification results in Figure 42 show biased estimates and increased uncertainty for all six longitudinal parameter estimates as compared to the baseline calm atmosphere test points 6-8.  The baseline parameter identification calm atmosphere test points 6-8 are calculated using SIDPAC lesq.m function. The parameter identification results calculated with Methods II-VI are compared to the baseline calm atmosphere test points. 
[bookmark: _Toc361522239]Method II



Method II represents the results calculated using the RTPID algorithm proposed by Morelli [10] and SIDPAC rtpid.m function. The results plotted in Figure 42 show small improvements for and   stability derivatives. The estimates of the remaining stability and control derivatives remain within the error bars of Method I and are a poor comparison to the calm atmosphere test points 6-8.
[bookmark: _Toc361522240]Method III

Method III represents the results calculated using the RTPID algorithm in Method II and a constant time delay to the airflow angle α regressor.  A constant time delay was used because it is easy to implement in real time: 

 										      (66)
where,

	= distance between α measurement position and center of gravity (assumed constant)

	= true airspeed 
and it does not require spectral estimation as explained in Chapter III. Spectral estimation is implemented in Method IV. A time delay of 0.085 seconds was used in this calculation. This time delay corresponds to an average airspeed of 62 meters per second and a distance from the airflow angle measurement position to the center of gravity of 5.3 meters.




The results in Figure 42 show improvements for all estimates in comparison to Method I and Method II. The estimates for  resulted in the largest improvement because angular velocity model parameters are most susceptible to time delays [66]. Correcting the airflow angle α regressor for time delay τ improved the remaining stability and control derivatives. This includes small improvements for and  stability derivatives and good agreement between light atmospheric turbulence and calm atmosphere for  stability and control derivatives.
[bookmark: _Toc361522241]Method IV

Method IV represents the results calculated using Method II and a time delay as a function of frequency and a scale factor as a function of frequency (These functions are detailed below). The results plotted in Figure 42 do not show any improvements over Method III. In fact, the results appear to have additional biasing and uncertainty. This is due to the scatter associated with spectral estimation in Figure 43 and Figure 48. The scatter below 0.5 Hz is associated with piloted inputs and is expected since the pilot is trying to excite the aircraft’s short period response (approximately 0.5 Hz for the Twin Otter). Additionally, as will be shown next, this approach does not facilitate real time implementation. In other words, the spectral estimation must be known a priori. The following figures and explanations summarize the spectral estimation of time delay and scale factor as a function of frequency.  A detailed derivation is presented in APPENDIX 2.

Figure 43 depicts the time delay as a function of frequency. The time delay is caused by the separation of the nose boom mounted airflow angle measurement position and the center of gravity. The magnitidue of the time delay represents the correction required to calculate the true angle of attack from measured data. The time delay, τ , is estimated by the phase lag between the measured angle of attack (nose boom) and the normal force coefficient (calculated by an inertial measurement system and corrected to the center of gravity). Unfortunately, the duration of test point 4 was 30 seconds and insufficient for spectral estimation. Data was gathered for all test points in the data record, approximately 400 seconds out of 2.5 hours, and used to estimate the phase spectrum in Figure 43. Data gathered for all test points will be referred to as forced oscillations (oscillations caused by pilot inputs) in atmospheric turbulence. Oscillations caused strictly by atmosphere turbulence will be referred to as atmospheric turbulence oscillations. The time delay estimation in Figure 43 used forced oscillations data.
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[bookmark: _Ref354432986][bookmark: _Toc361438008]Figure 43. Time Delay Estimation

The time delay calculation is

								      (67)
where the phase spectrum is the cross-spectrum of the lift coefficient (calculated from inertial measurements at the aircrafts center of gravity) and the angle of attack (measured on the noseboom of the aircraft), calculated using fast Fourier transforms, logarithmically spaced bins, and segment averaging. The parameter fk is the average frequency for each logarithmically spaced bin. Time delay derivation details and numerical calculations are included in APPENDIX 2 and APPENDIX 3.






The time delay calculation Eq. (67) is compared in Figure 44 using forced oscillations in atmospheric turbulence and atmospheric turbulence oscillations. 

[image: ]
[bookmark: _Ref354433319][bookmark: _Toc361438009]Figure 44. Time Delay Comparison


In Figure 44, the time delay for both data sets is almost identical from 2.0 Hz to 4.0 Hz. From 0.01 to 0.2 Hz both data sets show large differences. This is due to normal pilot inputs throughout the course of the flight. From 0.2 Hz to 0.5 Hz the time delay is less due to forced oscillations. The same effect is depicted from 0.5 to 2.0 Hz. At the aircraft’s short period frequency, 0.5 Hz, the time delay is approximately zero seconds. This corresponds to the pilots doublet input 0.2 to 0.4 Hz in Figure 45. In other words, near frequencies where the greatest pilot input is expected, the time delay is less. This coincides with the elevator power spectral density from 0.2-0.4 Hz, 0.8-1.2 Hz, and 1.5-1.9 Hz as shown in Figure 45.

[image: ]
[bookmark: _Ref354433420][bookmark: _Toc361438010]Figure 45. Elevator Power Spectral Density

This is analogous to the overpower technique described by Morelli [48] and discussed in Chapter II. However, Ref. [48] testing used multi-sine orthogonal inputs from 0.1-2.0 Hz which lessened (overpowered) the time delay over a wider frequency range than in manually piloted Twin Otter tests.  If multi-sine orthogonal inputs from 0.1-2.0 Hz had been used in Twin Otter tests it is hypothesized that the time delay would approach zero across the same frequency range. The upwash correction as a function of frequency will be discussed next. Additionally, it will be shown that although the time delay in light atmospheric turbulence can be overpowered, the same is not true for the upwash correction as a function of frequency. 

In order to discuss the upwash correction as a function of frequency, a brief overview is provided. This includes a steady state upwash model, an angle of attack measurement model, and a discussion on the slope of the lift curve slope from unsteady aerodynamics. Several assumptions and limitations are presented. A detailed derivation is presented in APPENDIX 2.

Steady state upwash model

The induced angle  due to upwash at the measurement position ahead of the wing and on the longitudinal axis of the aircraft is

								                   (68)

where  is the free stream angle of attack,  is the zero lift angle of attack, r [60] is the along-airstream distance between the measurement position and the aerodynamic center of the wing, c is the effective chord length of the wing, and , is the lift curve slope. The factor  in  is equal to  for an elliptical wing. This factor will be less for the Twin Otter’s rectangular wing with an aspect ratio of 6.

Angle of attack measurement model

									      	      (69)

where the measured angle of attack, α, is the addition of the free stream angle of attack and the upwash induced angle.

Lift curve slope from unsteady aerodynamics


The frequency response of a thin wing with infinite span to a sinusoidal gust in the direction of flight is the Sears function [62, 63]. The Sears function assumes unsteady two-dimensional incompressible potential flow and it assumes that atmospheric turbulence is sinusoidal and constant in span (1-D atmospheric turbulence).  The two dimensional assumption limits the analysis to wings of infinite span. The incompressible assumption, M < 0.3 [68], is not limiting since the Twin Otter’s speed range does not exceed a Mach number of 0.3. The potential flow assumption implies that this flow is an inviscid irrotational flow. This has direct consequences in the applicability of potential flow theory. In flow regions where vorticity is important (viscous effects), such as boundary layers and wakes, potential flow theory is not applicable. Additional limitations due to incompressible potential flow, such as erroneously predicting zero drag on an object moving through an infinite fluid at rest, are noted but not applicable to this work.  Potential flow is useful in this work since its focus is the flow outside of the boundary layer for an un-stalled wing. The assumption that atmospheric turbulence is constant in span is limiting since it has been shown that atmospheric turbulence is isotropic in the inertial sub-range [69]. In this range, which extends from eddies of hundreds of meters to millimeters, energy is transferred from larger to smaller eddies without loss.

Additional theoretical work by Diederich [70] and Filotas [71] on finite wings relaxed several limitations by taking into account the spanwise correlation of the local upwash velocities and isotropic atmospheric turbulence. Both analyses, however, have been based upon the approximation that the spanwise lift distribution due to gusts has an assumed shape, i.e., rectangular or elliptical, respectively. Therefore, both analyses do not take into account the variation of the spanwise lift distribution according to the frequency of gusts, aspect ratio, and sweep angle.







In the work by Okubo [72], it is shown that the lift distribution has an elliptical shape when the reduced frequency, where, is less than one but tends to become uniform along the span as the frequency  increases above one for rectangular planforms. As long as linearized potential flow theory is applicable, the response function of a finite wing to sinusoidal gusts approaches the two dimensional Sears function as the reduced frequency becomes greater than 0.5. The response is much more sensitive to changes of reduced frequency  at higher Mach numbers  and sweep angles [72].




Therefore, if the reduced frequency  is greater than 0.75 (Twin Otter airspeed range corresponds to) and the wing planform is nearly rectangular (Twin Otter wing is rectangular with an aspect ratio of 6); the power spectral density of the lift force arising from atmospheric turbulence can be evaluated by Figure 46. Figure 46 relates the Sears function (2-D Atmospheric Turbulence) to isotropic atmospheric turbulence using the lift coefficient power spectral density (PSD) vs. the reduced frequency.
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[bookmark: _Ref354865791][bookmark: _Ref354865781][bookmark: _Toc361438011]Figure 46. Validity of one-dimensional atmospheric turbulence

The work by Okubo [72] is based on numerical results using the lifting surface method [73, 74, 75, 76]. The Doublet Lattice method (a lifting surface method) [77, 78, 79] is the most popular unsteady subsonic flow and is widely used throughout industry [80]. Lifting surface methods are based on incompressible and compressible potential flow. Doublet Lattice methods are predominantly based on compressible potential flow and are limited to Mach numbers less than 0.8. 

In the case of an aerodynamic response to a sinusoidal gust, the slope of the lift curve is given by Ref. [71] as:

 										      (70)

where  is a generalized Sears response function, which includes the effect of the finite aspect ratio, A, and the effect of the spanwise structure of turbulence. The wavenumbers   and  correspond to the along-airstream and spanwise directions, respectively. Reference [71] explains the calculation of wavenumbers   and . 

Therefore, in order to estimate  , an estimate of the Sears response function is required.  

							                   (71)

The mathematical details of estimating the Sears response function are included in APPENDIX 2 and numerical calculations are included in APPENDIX 3. The frequency scale used in Figure 47 is the reduced frequency  based on the half chord because the Sears function depends on this parameter. Figure 47 shows the measured response function at frequencies above approximately 0.1 Hz because at lower frequencies there are contributions other than atmospheric turbulence (pilot inputs).

[image: ]
[bookmark: _Ref354434065][bookmark: _Toc361438012]Figure 47. Sears 2-D Response Function Estimation



Once the Sears response function is estimated, equation (69) is used to calculated the slope of the lift curve. The upwash is then calculated as , where  are calculated as previously defined. The angle of attack upwash correction is explained by examining a sensor model:

								      (72)
where,

 = angle of attack bias

 = measured angle of attack

 = true angle of attack


In Figure 48, the vertical axis represents the correction required to calculate the true angle of attack from measured data.

			           					      (73)

The frequency scale is the reduced frequency kb based on the half wing span where  is the angular frequency, b is the wingspan, and U is the true airspeed.
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[bookmark: _Ref354434278][bookmark: _Toc361438013]Figure 48. Angle of Attack Upwash Correction


At low frequencies the scale factor is approximately 0.75 and increases to 0.90 as kb approaches 2.0. A kb value of 2.0 (using the DHC-6 Twin Otter wing span and 110 knot cruise airspeed) corresponds to approximately 2.0 Hz. Therefore, over the frequency range of interest for rigid body aircraft dynamics (0.1 to 2.0 Hz), the scale factor changes from 0.75 to 0.90 due to atmospheric turbulence. The angle of attack upwash correction is compared in Figure 49 using forced oscillations in atmospheric turbulence and atmospheric turbulence oscillations. 
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[bookmark: _Ref354522807][bookmark: _Toc361438014]Figure 49. Upwash Correction Comparison


In Figure 49, the upwash correction for both data sets is similar from 0.8 Hz to 8.0 Hz. Although Figure 45 (elevator power spectral density) showed maximum energy at 0.2-0.4 Hz, 0.8-1.2 Hz, and 1.5-1.9 Hz it does not affect the upwash correction above 0.8 Hz. This result is significantly different from the time delay comparisons in Figure 44 and suggests that the upwash correction as a function of frequency cannot be overpowered during light atmospheric turbulence. Additional flight tests in light atmospheric turbulence with various input amplitudes are required to validate this hypothesis. From 0.01 to 0.8 Hz both data sets show large differences. This is due to normal pilot inputs throughout the course of the flight and doublet inputs at approximately 0.4 Hz. 



[bookmark: _Toc361522242]Method V

Represents the results calculated using the RTPID algorithm, a constant time delay, and a scale factor as a function of frequency. In this method, the scale factor as a function of frequency is calculated using the theoretical Sears response function instead of spectral estimation (Method IV). 

The results plotted in Figure 42 for callout 5) show the best estimates over all other approaches and compare very well to the no turbulence test points 6-8. In fact, the bias associated with time domain equation error estimates is all but eliminated. These results validate the hypothesis and additionally show that the “usual” model structure is adequate.

In order to facilitate a real time implementation and minimize the scatter observed in Figure 43 and Figure 48 the following assumptions are made. First, the time delay is constant and not a function of frequency. In test point 4 the average airspeed is 62 meters per second and the distance from the airflow angle measurement position to the center of gravity is 5.3 meters. This results in a time delay of 0.085 seconds. This calculation is easily implemented in real time by calculating a running airspeed average over a pre-determined length of time.  A thirty second window worked well for this analysis. The distance from the airflow angle measurement position to the center of gravity is assumed constant. Second, the measured Sears response function is replaced by the theoretical Sears response function.  Figure 50 compares the measured Sears response function to the theoretical Sears and Theodorsen [81] functions. The difference between the Sears and Theodorsen functions is that the Theodorsen function represents forced (e.g. maneuver) oscillations in a calm atmosphere whereas the Sears function represents a sinusoidal gust (atmospheric turbulence oscillation). The sinusoidal assumption correlates with continuous atmospheric turbulence. However, atmospheric turbulence contains both continuous atmospheric turbulence and gusts. In this method, it is assumed that the magnitude of light atmospheric turbulence is conservative with respect to light atmospheric gusts. In general, atmospheric turbulence oscillations are characterized by turbulence eddies travelling from the nose to the wing tip and along the wing chord, however, forced oscillations are not eddies, and the same oscillation occurs in all parts of the aircraft. Using the theoretical sears function eliminates the scatter of the measured Sears response function and relates well to the measured response function using spectral estimation.
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[bookmark: _Ref354434677][bookmark: _Toc361438015]Figure 50. Response Function Comparison



Third, the theoretical Sears response function is used to calculate the upwash defined by Eq. (69) and in turn calculate the angle of attack upwash correction . The upwash correction is anchored to the Twin Otter by matching the steady state upwash correction. NASA provided a steady state angle of attack upwash correction of 0.85. The steady state upwash correction along with other air data calibrations are typically first up in a flight test program. Therefore it is a reasonable assumption that this data point would be availabe for subsequent parameter identification test points. This correction is depicted in Figure 51.
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[bookmark: _Ref354434795][bookmark: _Toc361438016]Figure 51. Angle of Attack Upwash Correction Comparisons


These three assumptions are used to formulate an approach that is implemented in real time. 
[bookmark: _Toc361522243]Method VI



Method VI represents the results calculated using the state of the art extended EKF algorithm discussed in Chapter II. Results in Figure 42 do not show improvements for parameter estimates using Method VI in comparison to Method V. The only exception is the parameter estimate. This is expected because the control derivatives are based on measurements without errors. The estimates for  resulted in the largest degradation (outside of the standard plot scale) because angular velocity model parameters are most susceptible to time delays [66] and are not accounted for in the extended EKF. In general, the parameter estimates using Method V are superior to the state of the art.
[bookmark: _Toc361522244]Evaluation of Test Points 2 and 12

Figure 52 plots the longitudinal input and outputs during test point 12 in light atmospheric turbulence without icing.  The angle of attack (α) and normal acceleration (az) time histories show traces of atmospheric turbulence after the doublet input at 24 seconds. Before 24 seconds there are no traces of atmospheric turbulence in test point 12. During test point 12, the aircraft’s angle of attack response to a doublet was greater than the response caused by atmospheric turbulence. During the doublet input the aircraft experienced ± 0.25 g’s. 

In contrast to test point 4, test point 12 experiences atmospheric turbulence after the doublet input. This is an important contrast and was chosen to aid in the validation of Method V. In order to improve the robustness of Method V, it is important to know when to apply the time delay and upwash corrections. Test point 4 validated the need to apply a time delay and upwash correction if atmospheric turbulence occurred during the doublet input. Test point 12 will show that it is not necessary to apply a time delay and upwash correction if the doublet input occurred in a calm atmosphere and the aircraft subsequently entered into atmospheric turbulence. This statement assumes that the icing conditions do not change between test points. Operationally this can be verified by the aircraft’s ice detection and measurement equipment.
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[bookmark: _Ref355036863][bookmark: _Toc361438017]Figure 52. Test point 12 input and output flight data


Figure 53 depicts longitudinal parameter identification estimates for test point 12 using the six different methods discussed.  Test points 6-8 are plotted as a baseline reference with green markers. Two sigma error bars (95.5%) are plotted for each estimate. The parameter estimates and two sigma error bards for all methods are included in APPENDIX 4. 


In general, Method II estimates the best results because it does not include a time delay and an upwash correction. Method II is superior to Method I because it includes automatic filtering as discussed in Chapter II. Method II is superior to Method’s III, IV, and V because each of these methods implements a time delay and an upwash correction. The time delay and upwash correction are caused by atmospheric turbulence, in the absence of atmospheric turbulence, these corrections should not be applied. This is an important point and is implemented in the final real time parameter estimation methodology.  Method II is superior to Method VI (state of the art) in nearly every case. Method VI is tuned for atmospheric turbulence. If Method VI detects atmospheric turbulence, the process noise weights the atmospheric turbulence data over the calm atmosphere data. This process degrades the final Method VI results. The estimates for  resulted in the largest degradation (outside of the standard plot scale), because angular velocity model parameters are most susceptible to time delays [66] and are not accounted for in the extended EKF.
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[bookmark: _Ref355038252][bookmark: _Toc361438018]Figure 53. Test point 12 Light Atmospheric Turbulence without Icing
Figure 54 plots the longitudinal input and outputs during test point 2 in the lightest atmospheric turbulence and greatest icing of all three test points analyzed.  The angle of attack (α) and normal acceleration (az) time histories show traces of atmospheric turbulence throughout the data run. During test point 2, the aircraft’s angle of attack response to a doublet was greater than the response caused by atmospheric turbulence. During the doublet input the aircraft experienced ± 0.4 g’s. 

This test point was chosen because it was desired to accurately estimate the differences to aircraft stability and control coefficients in icing conditions as described in the introduction.
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[bookmark: _Ref355039975][bookmark: _Toc361438019]Figure 54. Test point 2 input and output flight data




Figure 55 depicts longitudinal parameter identification estimates for test point 2 using the six different methods discussed.  Test points 6-8 are plotted as a baseline reference with green markers. Two sigma error bars (95.5%) are plotted for each estimate. The parameter estimates and two sigma error bards for all methods are included in APPENDIX 4. 





Since atmospheric turbulence is present throughout the data record, the results of Method V are preferred over all other methods. In this case, the baseline results are used as a reference to the un-iced aircraft. Any differences from baseline test points 6-8 are attributed to icing accretion and not errors due to atmospheric turbulence. As expected, icing causes degradation in and very little change in the remaining stability and control parameters. The only exception is   or lift damping stability derivative. This was unexpected, but because the product of this derivative times its regressor is an order of magnitude less than  it is difficult to estimate and does not significantly contribute to the aerodynamic model. 



Method VI results for are consistent with the analysis of test points 4 and 12. The estimates for  resulted in the largest degradation (outside of the standard plot scale) because angular velocity model parameters are most susceptible to time delays [66] and are not accounted for in the extended EKF.
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[bookmark: _Ref355040390][bookmark: _Toc361438020]Figure 55. Test point 2 Light Atmospheric Turbulence in Icing



[bookmark: _Toc361522245]Summary and conclusions of estimation results


In summary, this chapter investigated six different parameter identification methods to analyze flight data in atmospheric turbulence with and without icing. Atmospheric turbulence was classified by using the internationally accepted MIL-F-8785C atmospheric turbulence model. Using this metric it was determined that light atmospheric turbulence was the highest level of atmospheric turbulence recorded. 

Three test points were selected as baseline references and three test points were selected for analysis and comparison. Test point 4 represents all surfaces de-iced in light atmospheric turbulence, Test point 2 represents all surfaces iced in light atmospheric turbulence, and Test point 12 represents all surfaces de-iced in light atmospheric turbulence. Test point 12 represents a case where a parameter identification input was applied in calm atmosphere, and the aircraft subsequently experienced light atmospheric turbulence.

Each test point was analyzed using all six methods. It was determined that Method V, RTPID with a fixed time delay and a theoretical upwash correction anchored on flight test calibrations, outperformed all other methods including the state of the art (Method VI). Additionally, it was determined that the time delay and upwash corrections can be applied in real time using a running vertical velocity standard deviation calculation for guidance. The vertical velocity standard deviation calculation accurately detects the presence, magnitude, and required correction for parameter identification in light atmospheric turbulence. Although Method V is based on unsteady potential flow and has several limitations, these limitations are not restrictive in the case of the Twin Otter aircraft. Additional data is needed in moderate and severe atmospheric turbulence to validate the method.


[bookmark: _Toc361522246]Chapter VI
Future studies
[bookmark: _Toc361522247]Sweep wing corrections

The methodology developed in Chapter 5 Method V assumed that the wing was rectangular. This is a good assumption for the Twin Otter aircraft used in this work. Okubo [72] showed that for reduced frequency values representative of flight the lift distribution was rectangular. This permitted the use of work by Diederich [70] to estimate the airflow angle  upwash correction as a function of frequency for isotropic atmospheric turbulence. However, Okubo [72] also showed that the lift distribution is not rectangular for a swept wing at any Mach number. Additional analytical work is required to determine the corrections required for swept wings and the Mach number limitations for rectangular wings in the present work.
[bookmark: _Toc361522248]Wing Tip Alpha Airflow Vane corrections

This work assumed that the airflow angle α measurement was mounted on a nose boom. Additional analytical and experimental work is needed to correct measurements from a wing tip mounted boom. 
[bookmark: _Toc361522249]Moderate and Severe Atmospheric Turbulence

This work was limited to light atmospheric turbulence. Additional flight test data is required for moderate and severe atmospheric turbulence in order to test the validity of Method V and its limitations. The problem is further compounded by rarity of moderate and severe atmospheric turbulence. Additionally, severe atmospheric turbulence threatens the safety of the crew and the aircraft.



[bookmark: _Toc361522250]Beta Airflow Vane corrections


This work was limited in scope to longitudinal parameter identification. Figure 56 and Figure 57 show that atmospheric turbulence has similar effects on lateral and directional stability and control derivatives. Figure 56 shows parameter estimation results from T-2 flight test data using equation-error in the frequency domain. Each marker represents a different run, and only the last estimate of each real-time parameter estimation run is shown. The error bars represent or 95.5% confidence bounds. A total of nine runs are represented; six in high and three in low atmospheric turbulence. 

T-2 FLT 15 C21 WT04
(High Turbulence)
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[bookmark: _Ref355296496][bookmark: _Toc361438021]Figure 56. Lateral-directional effects of atmospheric turbulence on T-2 modeling results
(Dr Eugene A. Morelli, personal communication, April 24, 2013 see also Refs.  [48] and [56])
		


Figure 57 shows additional lateral and directional parameter estimation results from T-2 flight test data using equation-error in the frequency domain. 
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[bookmark: _Ref355296511][bookmark: _Toc361438022]Figure 57. Additional lateral-directional effects of atmospheric turbulence on T-2 modeling results
 (Dr Eugene A. Morelli, personal communication, April 24, 2013 see also Refs.  [48] and [56])
		




Additional analytical work is required in order to determine how to correct the bias and scatter in the stability derivatives based on airflow angle β in Figure 56. Based on the findings in this work, it is hypothesized that once the airflow angle β regressor is corrected RTPID will yield the same aerodynamic model inside and outside of atmospheric turbulence.
[bookmark: _Toc361522251]Chapter VII
Conclusions and Recommendations

Several practical issues related to real-time parameter estimation for a linear longitudinal dynamics model in atmospheric turbulence were examined and discussed. These issues included the frequency response of airflow angles vanes, the structural response of the air data boom, wing aerodynamic response, and aerodynamic model structure in atmospheric turbulence as potential sources of colored noise. An airflow vane dynamic model was proposed to investigate (via simulation) contributions to colored noise. Frequency based airflow angle α calculations showed that the air data boom was insensitive to vibrations. It was determined that a major flow distortion, which seriously affects the vertical wind velocity measurements near the nose of an aircraft, is the frequency-dependent upwash and time delay. These are shown to be the result of (1) not taking into account the decrease in lift and subsequent decrease in upwash correction with eddy frequency caused by the response of the wing vortex system to atmospheric turbulence, (2) the variation of spanwise loading with eddy frequency, and (3) the longitudinal distance between the angle of attack sensor and the center of gravity. Flight data analysis of the lift coefficient verified the decrease in lift coefficient and angle of attack in atmospheric turbulence in comparison to a calm atmosphere at the same flight condition. Data compatibility methods verified the existence of time delay in the airflow angle α measurement. Lastly, an alternative aerodynamic model structure was suggested with additional atmospheric turbulence coefficients.
[bookmark: _Toc361522252]Simulated Data

Practical issues were examined using data from a Twin Otter DHC-6 longitudinal linear simulation, with realistic noise sequences added to the computed aircraft responses. This allowed a clear view of the effect of each source of colored noise to the modeling problem, because the true values of the model parameters were known. This approach was used initially to show that real-time parameter estimation can be done accurately in all atmospheric turbulence conditions if the angle of attack measurement is accurate. The effects of the frequency response of airflow angle vanes and the wing aerodynamic response in atmospheric turbulence as potential sources of colored noise were studied. It was determined that vane dynamics do not substantially contribute to the scatter in the estimates, because all of the added dynamics are outside the range of frequencies analyzed. Corrupting the angle of attack by a frequency dependent magnitude and time delay corrupted the stability and control derivatives as shown in the problem statement (Figure 2 and Figure 3). Additionally, it was shown that the classical aerodynamic model structure was not a major source of colored noise. 
[bookmark: _Toc361522253]Flight Data

Flight test data from the NASA Glenn DHC-6 Twin Otter aircraft were used to evaluate six parameter identification methods in atmospheric turbulence with and without icing. Atmospheric turbulence was classified by using the internationally accepted MIL-F-8785C atmospheric turbulence model. Using this metric it was determined that light atmospheric turbulence was the highest level of atmospheric turbulence recorded. 

Three test points were selected as baseline references and three test points were selected for analysis and comparison. Each test point was analyzed using all six methods. It was determined that Method V, RTPID with a fixed time delay and a theoretical upwash correction anchored on calm atmosphere flight test calibrations, outperformed all other methods including the state of the art. Additionally, it was determined that the time delay and upwash corrections can be applied in real time using a running vertical velocity standard deviation calculation for guidance. The vertical velocity standard deviation calculation accurately detects the presence, magnitude, and required correction for parameter identification in light atmospheric turbulence. Although Method V is based on unsteady potential flow and has several limitations, these limitations are not restrictive in the case of the Twin Otter aircraft due to its rectangular wing and speed limitation.

Based on these findings, several practical recommendations for future flight testing in atmospheric turbulence are suggested. First, mount the air data boom at the nose of the aircraft to minimize the effect of wing-bound and wing-tip vortices. Second, an upwash and time delay calibration as a function of frequency is required for accurate airflow angle α measurements. Third, for frequencies of interest, 0.1 to 2.0 Hz, either airflow vanes or pressure based measurements are adequate. Fourth, currently available COTS turbulence sensors do not offer significant advantage over well calibrated research flight test instrumentation, other than convenience. Fifth, additional data is required in moderate and severe atmospheric turbulence to validate Method V.

In summary, this work has expanded the state of the art with the following contributions:

1) A major source of colored noise in the explanatory variables for real time parameter identification in atmospheric turbulence is demonstrated and explained. The explanation includes the original derivation first reported in another field of science – airborne wind measurements for atmospheric science – and a detailed unreported derivation.
2) This work demonstrates how to correctly simulate colored noise for longitudinal parameter identification created by atmospheric turbulence on the airflow angle α explanatory variable.
3) It demonstrates that once airflow angle α is corrected, other sensors do not need additional corrections for longitudinal parameter identification. This assumes that accelerations, rates, and attitudes are measured at the center of gravity. This also assumes that the control surface deflections are measured without errors. Both are realistic assumptions in flight test aircraft.
4) It demonstrates that the usual aerodynamic model structure for longitudinal parameter identification is sufficient, and a new model structure is not required.
5) It develops a simple real time methodology that complements the state of the art real time parameter identification method in a steady atmosphere with minimal a priori information.
6) It dramatically improves real time parameter estimation parameters and parameter error measures in atmospheric turbulence over the current state of the art.
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function rtout = rtpid_totter(fdata,dt,lpest,lmod,linit,p0,crb0,kbflag)
%
%  RTPID_TOTTER Real-time parameter estimation for the Twin Otter.
%
%  Usage: rtout = rtpid_totter(fdata,dt,lpest,lmod,linit,p0,crb0);
%
%  Description:
%
%    Real-time parameter estimation using sequential
%    least squares equation-error in the frequency domain.  
%    Transformation of time-domain data into the 
%    frequency domain is done using a recursive 
%    Fourier transform.  Inputs specifying a parameter
%    estimate update lpest, modeling choice lmod,  
%    initialization linit, initial estimated parameter 
%    vector p0, and initial estimated parameter covariance 
%    matrix crb0, are optional.  
%
%  Input:
%    
%    fdata = flight data array in standard configuration.
%       dt = sampling time, sec.
%    lpest = parameter estimation flag:
%            = 0 to omit the parameter estimation (default)
%            = 1 to calculate parameter estimates
%     lmod = modeling flag:
%            = 0 for non-dimensional derivatives (default) 
%            = 1 for dimensional derivatives 
%    linit = initialization flag:
%            = 0 for normal operation (default)
%            = 1 to initialize
%       p0 = initial parameter vector (default=zero vector).
%     crb0 = initial parameter covariance(default=10^6*identity matrix).
%
%  Output:
%
%    rtout = data structure:
%    rtout.y    = model output using current estimated parameters.
%    rtout.p    = current estimated parameter vector.
%    rtout.serr = current estimated parameter standard error vector.
%    rtout.s2   = current model fit error variance estimate.  
%    rtout.Z    = measured output Fourier transform.
%    rtout.U    = measured input Fourier transform.
%    rtout.X    = regressor matrix Fourier transform.
%    rtout.f    = frequency vector for the Fourier transforms, Hz.
%    rtout.zf   = low-pass filtered output vector.
%    rtout.uf   = low-pass filtered input vector. 
%    rtout.xf   = low-pass filtered regressor vector. 
% 
%

%    Calls:
%      rtfilt.m
%      rft_BM.m
%      lesq.m
%
%    Authors:  Eugene A. Morelli (EAM) & Borja Martos (BM)
%
%    History:  
%      08 Mar  2007 - Created and debugged, EAM.
%      02 Jul  2007 - Modified output format, EAM.
%      22 Oct  2007 - Updated to include non-dimensional case, EAM.
%      03 Mar  2008 – Dec 2012 Modified to output longitudinal non %dimensional derivatives, updated inputs and outputs, updated recursive %Fourier transform function call, BM. 
%
%  Copyright (C) 2007  Eugene A. Morelli
%
%  This program carries no warranty, not even the implied 
%  warranty of merchantability or fitness for a particular purpose.  
%
%  Please email bug reports or suggestions for improvements to:
%
%      e.a.morelli@nasa.gov
%
persistent w b a dataf0
persistent Z0 U0 X0 C0
%
%  Set defaults.
%
if nargin < 3 | isempty(lpest)
  lpest=0;
end
if nargin < 4 | isempty(lmod)
  lmod=0;
end
if nargin < 5 | isempty(linit)
  linit=0;
end
%
%  Constants.
%
dtr=pi/180;
g=32.174;
jay=sqrt(-1);
%
%  Define outputs, inputs, and regressors. 
%
  sarea=fdata(77);
  cbar=fdata(79);
  bspan=fdata(78);
  c2v=cbar/(2*fdata(2));
  b2v=bspan/(2*fdata(2));
  qs=fdata(27)*sarea;
  qsc=qs*cbar;
  qsb=qs*bspan;
  av=fdata([5:7])*dtr;
  mass=fdata(48);
  Ixx=fdata(49);
  Iyy=fdata(50);
  Izz=fdata(51);
  Ixz=fdata(52);
  k1=mass*g/qs;
  [CX,CY,CZ,CD,CYw,CL,CT_X]=compfc(fdata);
  z=[fdata(4)*dtr,av(2)*c2v,fdata(11)*k1,CL,...
     fdata(3)*dtr,[av(1),av(3)]*b2v,fdata(12)*k1,...
     av(2)*Iyy/qsc,...
     (av(1)*Ixx-av(3)*Ixz)/qsb,...
     (av(3)*Izz-av(1)*Ixz)/qsb,...
     (av(1)*av(3)*(Ixx-Izz)+(av(1)*av(1)-av(3)*av(3))*Ixz)/qsc,...
     (av(2)*av(3)*(Izz-Iyy)-av(2)*av(1)*Ixz)/qsb,...
     (av(1)*av(2)*(Iyy-Ixx)+av(2)*av(3)*Ixz)/qsb]';
  u=dtr*[fdata(14),fdata(15),fdata(16),fdata(17)]';
  lonindx=[1,2,15];

x=[z;u];
%
%  Dimensions.
%
no=length(z);
ni=length(u);
nr=length(x);
np=length(lonindx)+length(lonindx);
%
%  Number of model outputs, or number of equations.
%
nmo=2;
%
%  Initialization.
%
if linit==1
  fmin=.1;
  fmax=2;
  df=0.01;
  f=[fmin:df:fmax]';
  w=2*pi*f;
  nw=length(w);
%
%  Fourth-order high-pass butterworth filter coefficients.
%  Filter is designed for a cut-off frequency of 0.02 Hz. 
%  Hard code the filter coefficients.  
%
  b=[9.967216337145971e-001,-3.986886534858388e+000,5.980329802287582e+000,-3.986886534858388e+000,9.967216337145971e-001];
  a=[1.000000000000000e+000,-3.993432499059752e+000,5.980319054621965e+000,-3.980340570637141e+000,9.934540151146954e-001];
%
%  Initialize the high pass filters.
%
  dataf0=[z;u];
  dataf=rtfilt(b,a,[z;u]-dataf0,1);
  zf=dataf(1:no);
  uf=dataf(no+1:no+ni);
  xf=[zf;uf];
%
%  Recursive Fourier transform storage.
%
  Z0=zeros(no,nw);
  U0=zeros(ni,nw);
  X0=zeros(nr,nw);
  Z=Z0;
  U=U0;
  X=X0;
  C0=exp(-jay*w'*0);
else
%
%  Recursive Fourier transform.
%
%  Allow for varying time step dt.
%
  dC=exp(-jay*w'*dt);
%
%  Compute the high pass filtered values of u and z.  
%  This is done to prevent pollution of the
%  frequency content by large biases in the 
%  time domain data.  Initial values of u and z
%  must be subtracted to start the filter properly.  
%
  dataf=rtfilt(b,a,[z;u]-dataf0,0);
  zf=dataf(1:no);
  uf=dataf(no+1:no+ni);
  xf=[zf;uf];
%
%  Update the recursive Fourier transform.
%
  [Z,C]=rft_BM(zf,dC,Z0,C0,kbflag);
  [U,C]=rft_BM(uf,dC,U0,C0,0);
  [X,C]=rft_BM(xf,dC,X0,C0,kbflag);
  Z0=Z;
  U0=U;
  X0=X;
  C0=C;
end
%
%  Check for a parameter estimation calculation. 
%
if lpest==1
%
%  Estimate dimensional or non-dimensional derivatives, 
%  according to lmod.  The characters .' mean transpose without 
%  complex conjugation.  
%
%  Equation-error parameter estimation.
%
  Ze=jay*w(:,ones(1,no)).*Z.';
  Xe=X.';

%
%  Non-dimensional derivatives.
%
    
%
%  Vertical force coefficient with CZq.
%
[YZ,pZ,crbZ,s2Z]=lesq(Xe(:,lonindx),Xe(:,4),0,p0(1:3),diag(crb0(1:3)));
    serrZ=sqrt(diag(crbZ));
    yZ=xf(lonindx)'*pZ;      
%
%  Pitching moment coefficient.
% [Ym,pm,crbm,s2m]=lesq(Xe(:,lonindx),Ze(:,9)+Xe(:,12),0,p0(4:6),diag(crb0(4:6)));
    serrm=sqrt(diag(crbm));
    ym=xf(lonindx)'*pm;    
%
%  Assemble the results.
%
  y=[yZ;ym];
  p=[pZ;pm];
  serr=[serrZ;serrm];
  s2=[s2Z;s2m];
else
  y=zeros(nmo,1);
  p=zeros(np,1);
  serr=zeros(np,1);
  s2=zeros(nmo,1);
end
f=w/(2*pi);
%
%  Assign the outputs.
%
rtout.y=y;
rtout.p=p;
rtout.serr=serr;
rtout.s2=s2;
rtout.Z=Z;
rtout.U=U;
rtout.X=X;
rtout.f=f;
rtout.zf=zf;
rtout.uf=uf;
rtout.xf=xf;
return
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A detailed derivation of the Sears 2-D function based on Ref. [60] for the upwash estimation from flight data is included in this appendix. This derivation includes a correction for non-elliptical lift distributions and a theoretical upwash calculation. Additional derivations are included for the time delay estimated from flight data and a theoretical time delay calculation.

Up-wash estimation from flight data
Equations are numbered based on Ref. [60].

									        (2)

										        (3)

									        (4)
and 

										      (4a)
Substitute equations (2), (4), and (5) into equation (3)

							      (4b)
For variations from an average state (primes):

								      (4c)
The free airstream angle is assumed to be sinusoidal gust traveling with Uα:

							      (4d)
At the angle of attack measurement location (x=0):

									      (4e)

At the leading edge of the wing (x=Δx):

					      (4f)

In the variations equation above the angle variation α’, which is measured at the radome (x=0), is actually the sum of α’f at x=0 and the upwash angle caused by α’f at, because the free airstream attack angle at the leading edge of the wing determines the bound vortex and the upwash angle (αu) as mentioned in the text before Eq. (5) in Ref. [60]:

						      (4g)
Using the last two equations (4f, 4g) we get Equation (5) in the Ref. [60].
First rearrange equation (4f)


Substitute into equation (4g)




Multiply the second term in the right hand side of equation (4g) by and solve for 

		Equation (5) in the reference paper

 				Equation (6) in the reference paper

Using equation (5) in the reference paper

							      (6a)
Substitute equation (6a) into equation (6)

 			Equation (7) in the reference paper
Solving for SG
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Once an estimate of the Sears function is calculated, the up-wash is calculated as:


Correction for non-elliptical lift distribution





At therefore








The value of  is estimated as where is the calibration factor for the upwash correction at low frequencies as estimated by maneuvers. This does two things 1) it is used to account for the difference from an elliptical wing (match the theoretical to measured Sears response function) and 2) it constraints  to as measured during calm atmosphere maneuvers.



From maneuvers in a calm atmosphere  and 



Therefore, in the upwash theoretical calculations presented in the next section.

Upwash theoretical calculation
Starting with equation (5) in the Ref. [60],



Take its Fourier transform without the time delay in the numerator because we are estimating at x=0 (measurement location) and not at x=dx (wing leading edge) as in the original derivation.



At




For all frequencies


therefore,






In order to calculate the upwash correction as a function of reduced frequency , the theoretical  value, measured  , and calculated  must be known.  

According to Ref. [72],



Time delay estimated from flight data


Time delay calculation
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APPENDIX 3

%
%  Time delay, Coherence, Sears function, and Ku calculations
%
%  Usage: No function calls required
%
%  Description:
%
%    Time delay and coherence is calculated using cross spectral
%    density functions. The Sears function is estimated based on input 
%    data and used to calculated Ku as a function of reduced frequency %    kb.  
%
%  Input: N/A
%    
%  Output:
%
%    Figure 1 – Time delay as a function of frequency (Hz)
%    Figure 2 – Coherence as a function of frequency (Hz)
%    Figure 3 – Sears function as a function of reduced frequency Kc
%    Figure 4 – Ku as a function of reduced frequency Kb
%
%  Calls: N/A
%
%  Author:  Borja Martos 
%
%  History:  
%      12 Jan 2012 - Created and debugged.
%
%  Copyright (C) 2012 Borja Martos
%
%  This program carries no warranty, not even the implied 
%  warranty of merchantability or fitness for a particular purpose.  
%
%  Please email bug reports or suggestions for improvements to:
%
%      bmartos@utsi.edu
%
clear all
clc
% GUI to select data set
[FileName,PathName] = uigetfile('*.mat','Select mat file');
load(fullfile(PathName,FileName))
% Cross spectral density calculations
[Pxy,freq]   = cpsd(aoa, CL,[],0,4096,50);
[Pxx,freqxx] = cpsd(aoa, aoa,[],0,4096,50);
[Pyy,freqyy] = cpsd(CL , CL,[],0,4096,50);
 
numBins=27;                          %define number of bins - log
binEdges=logspace(-2,1,numBins+1);   %define bin edges
[h,whichBin]=histc(freq,binEdges);
 

for i = 1:numBins
    flagBinMembers = (whichBin == i);
    binMembers = Pxy(flagBinMembers);
    binMean(i) = mean(binMembers);  %Mean of each bin - Cross Spectrum
    frqMembers = freq(flagBinMembers);
    frqMean(i) = mean(frqMembers);  %Mean of each bin - frequency
end
 
%Time delay Calculation
Kxy= real(binMean);
Qxy= imag(binMean);
pha  = atan2( -Qxy, Kxy );
dt=-pha./(2*pi*frqMean);
figure(1)
semilogx(frqMean,dt,'*','MarkerSize',5)
xlabel('frequency (Hz)')
ylabel('time delay (seconds)')
xlim([10^-2 10])
ylim([-1 1])
grid on
 
%Coherence Calculation
for i = 1:numBins
    flagBinMembers = (whichBin == i);
        binMembers = Pxx(flagBinMembers);
    binMean(i) = mean(binMembers); 
        binMembers1 = Pyy(flagBinMembers);
    binMean1(i) = mean(binMembers1); 
        binMembers2 = Pxy(flagBinMembers);
    binMean2(i) = mean(binMembers2); 
end
 
figure(2)
coh = binMean2.*conj(binMean2)./(binMean.*binMean1);
semilogx(frqMean,coh,'*','MarkerSize',5)
xlabel('frequency (Hz)')
ylabel('Coherence')
xlim([10^-2 10])
ylim([0 1])
grid on
 
%Sears function Calculation
kts2mps=0.514444;
Uavg=mean(U)*kts2mps;
HCL=(binMean2);
HAOA=(binMean);
k0=1/(pi^2);
dx=5.3; %meters
cbar=6.5*0.3048; %ft 2 meters
n=dx/cbar;
Sg=HCL./(2*pi*exp((-1i*2*pi*frqMean*dx)/Uavg).*((HAOA)-(HCL*(k0/n))));
figure(3)
kc=(2*pi*frqMean*cbar*0.5)/Uavg;
 

%Sears function Calculation Continued
[kcTHEORY,C,S2S0,H,kbTHEORY] = Sears2DTheodorsen(64);
semilogx(kc,abs(Sg),'*','MarkerSize',5)
xlabel('k_c=\omega*(c/2)/U')
ylabel('Amplitutde')
xlim([10^-3 1])
ylim([0 1])
grid on
hold all
semilogx(kcTHEORY,abs(S2S0),'*','MarkerSize',5)
semilogx(kcTHEORY,abs(C),'o','MarkerSize',5)
legend('Measured Response function','Sears','Theodorsen')
hold off
 
%ku Calculation
ku=2*pi*(k0/n)*abs(Sg);
ku_corr=1./(1+ku);
bspan=65*0.3048; %ft 2 meters
kb=(2*pi*frqMean*bspan*0.5)/Uavg;
figure(4)
semilogx(kb,ku_corr,'*','MarkerSize',5)
xlabel('k_b=\omega*(b/2)/U')
ylabel('(1+k_u)^-1')
xlim([10^-3 2])
ylim([0.7 1.05])
grid on
hold all
semilogx(kbTHEORY,abs(H),'o','MarkerSize',5)
legend('Measured','Sears Based')
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[bookmark: _Toc356339986]Table 7. Baseline reference parameters and confidence bounds
	
	Test Point
	Parameter
	Baseline Reference
	

	
	
	
	Estimate
	95% Confidence Bounds
	

	
	TP 6
	CLα
	6.31
	+/- 0.02
	

	
	
	CLq
	65.26
	+/- 0.97
	

	
	
	CLδe
	0.39
	+/- 0.03
	

	
	
	CMα
	-1.79
	+/- 0.01
	

	
	
	CMq
	-48.58
	+/- 0.66
	

	
	
	CMδe
	-1.74
	+/- 0.02
	

	
	



	TP 7
	CLα
	6.38
	+/- 0.01
	

	
	
	CLq
	68.78
	+/- 0.47
	

	
	
	CLδe
	0.49
	+/- 0.01
	

	
	
	CMα
	-1.89
	+/- 0.01
	

	
	
	CMq
	-51.28
	+/- 0.49
	

	
	
	CMδe
	-1.86
	+/- 0.01
	

	
	TP 8
	CLα
	6.43
	+/- 0.02
	

	
	
	CLq
	67.97
	+/- 1.26
	

	
	
	CLδe
	0.46
	+/- 0.03
	

	
	
	CMα
	-1.84
	+/- 0.01
	

	
	
	CMq
	-51.07
	+/- 0.63
	

	
	
	CMδe
	-1.84
	+/- 0.02
	

	
	Average
	CLα
	6.37
	+/- 0.02
	

	
	
	CLq
	67.34
	+/- 0.90
	

	
	
	CLδe
	0.45
	+/- 0.02
	

	
	
	CMα
	-1.84
	+/- 0.01
	

	
	
	CMq
	-50.31
	+/- 0.59
	

	
	
	CMδe
	-1.82
	+/- 0.02
	

	
	
	
	
	
	



[bookmark: _Toc355130440][bookmark: _Toc355299687][bookmark: _Toc356420658][bookmark: _Toc361521796][bookmark: _Toc361522260]The average of TP 6-8 stability and control coefficients are used to calculate the percent change in Table 8, Table 9, and Table 10. Percent change is defined as:


					


Table 8. Test point 2 parameters and confidence bounds

	Method
	Parameter
	Test Point 2

	
	
	Estimate
	% Change
	95% Confidence Bounds

	I
	CLα
	5.29
	-17.00
	+/- 0.16

	
	CLq
	52.28
	-22.37
	+/- 6.30

	
	CLδe
	0.02
	-95.83
	+/- 0.17

	
	CMα
	-1.35
	26.90
	+/- 0.07

	
	CMq
	-42.64
	15.25
	+/- 2.77

	
	CMδe
	-1.54
	15.21
	+/- 0.07

	II
	CLα
	5.27
	-17.27
	+/- 0.11

	
	CLq
	43.88
	-34.83
	+/- 5.85

	
	CLδe
	-0.22
	-149.65
	+/- 0.17

	
	CMα
	-1.32
	28.65
	+/- 0.05

	
	CMq
	-42.54
	15.45
	+/- 2.87

	
	CMδe
	-1.52
	16.04
	+/- 0.08

	III
	CLα
	5.36
	-15.85
	+/- 0.10

	
	CLq
	83.34
	23.77
	+/- 5.29

	
	CLδe
	0.41
	-8.50
	+/- 0.15

	
	CMα
	-1.36
	26.24
	+/- 0.05

	
	CMq
	-52.63
	-4.60
	+/- 2.72

	
	CMδe
	-1.69
	6.72
	+/- 0.08

	IV
	CLα
	6.15
	-3.53
	+/- 0.11

	
	CLq
	83.26
	23.65
	+/- 5.34

	
	CLδe
	0.39
	-12.67
	+/- 0.15

	
	CMα
	-1.56
	15.53
	+/- 0.06

	
	CMq
	-52.58
	-4.52
	+/- 2.74

	
	CMδe
	-1.69
	7.03
	+/- 0.08

	V
	CLα
	7.09
	11.21
	+/- 0.33

	
	CLq
	114.27
	69.70
	+/- 12.50

	
	CLδe
	-0.87
	-293.38
	+/- 0.31

	
	CMα
	-1.82
	1.40
	+/- 0.10

	
	CMq
	-61.00
	-21.25
	+/- 3.99

	
	CMδe
	-1.38
	24.08
	+/- 0.10

	VI
	CLα
	5.64
	-11.54
	+/- 0.03

	
	CLq
	5.90
	-91.24
	+/- 0.13

	
	CLδe
	0.08
	-82.23
	+/- 0.04

	
	CMα
	-1.71
	7.34
	+/- 0.01

	
	CMq
	-4.89
	90.28
	+/- 0.03

	
	CMδe
	-1.90
	-4.87
	+/- 0.01
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[bookmark: _Ref355130134][bookmark: _Toc356339988]Table 9. Test point 4 parameters and confidence bounds
	Method
	Parameter
	Test Point 4

	
	
	Estimate
	% Change
	95% Confidence Bounds

	I
	CLα
	5.20
	-18.39
	+/- 0.18

	
	CLq
	52.08
	-22.66
	+/- 6.06

	
	CLδe
	-0.01
	-102.14
	+/- 0.16

	
	CMα
	-1.39
	24.43
	+/- 0.07

	
	CMq
	-41.62
	17.28
	+/- 2.37

	
	CMδe
	-1.52
	16.33
	+/- 0.07

	II
	CLα
	5.37
	-15.77
	+/- 0.12

	
	CLq
	46.42
	-31.07
	+/- 5.85

	
	CLδe
	-0.16
	-134.70
	+/- 0.18

	
	CMα
	-1.44
	22.13
	+/- 0.06

	
	CMq
	-41.15
	18.22
	+/- 2.67

	
	CMδe
	-1.50
	17.40
	+/- 0.08

	III
	CLα
	5.52
	-13.33
	+/- 0.11

	
	CLq
	87.45
	29.87
	+/- 5.41

	
	CLδe
	0.53
	19.13
	+/- 0.16

	
	CMα
	-1.49
	19.30
	+/- 0.05

	
	CMq
	-52.15
	-3.66
	+/- 2.60

	
	CMδe
	-1.69
	7.06
	+/- 0.08

	IV
	CLα
	6.31
	-1.00
	+/- 0.13

	
	CLq
	87.29
	29.64
	+/- 5.50

	
	CLδe
	0.52
	15.22
	+/- 0.16

	
	CMα
	-1.70
	8.01
	+/- 0.06

	
	CMq
	-52.05
	-3.47
	+/- 2.63

	
	CMδe
	-1.68
	7.41
	+/- 0.08

	V
	CLα
	7.56
	18.65
	+/- 0.39

	
	CLq
	112.73
	67.42
	+/- 12.91

	
	CLδe
	-0.94
	-309.45
	+/- 0.34

	
	CMα
	-2.02
	-9.39
	+/- 0.13

	
	CMq
	-58.79
	-16.85
	+/- 4.23

	
	CMδe
	-1.29
	29.01
	+/- 0.11

	VI
	CLα
	5.64
	-11.54
	+/- 0.03

	
	CLq
	5.90
	-91.24
	+/- 0.13

	
	CLδe
	0.08
	-82.23
	+/- 0.04

	
	CMα
	-1.71
	7.34
	+/- 0.01

	
	CMq
	-4.89
	90.28
	+/- 0.03

	
	CMδe
	-1.90
	-4.87
	+/- 0.01





[bookmark: _Ref355130144][bookmark: _Toc356339989]Table 10. Test point 12 parameters and confidence bounds
	Method
	Parameter
	Test Point 12

	
	
	Estimate
	% Change
	95% Confidence Bounds

	I
	CLα
	5.82
	-8.70
	+/- 0.20

	
	CLq
	66.16
	-1.75
	+/- 6.74

	
	CLδe
	0.42
	-6.24
	+/- 0.18

	
	CMα
	-1.56
	15.35
	+/- 0.07

	
	CMq
	-47.75
	5.08
	+/- 2.18

	
	CMδe
	-1.79
	1.53
	+/- 0.06

	II
	CLα
	5.94
	-6.76
	+/- 0.11

	
	CLq
	65.63
	-2.54
	+/- 5.40

	
	CLδe
	0.36
	-20.62
	+/- 0.17

	
	CMα
	-1.61
	12.79
	+/- 0.06

	
	CMq
	-49.96
	0.70
	+/- 2.78

	
	CMδe
	-1.83
	-0.74
	+/- 0.09

	III
	CLα
	6.01
	-5.76
	+/- 0.11

	
	CLq
	106.85
	58.68
	+/- 5.70

	
	CLδe
	1.01
	126.21
	+/- 0.17

	
	CMα
	-1.65
	10.48
	+/- 0.05

	
	CMq
	-61.38
	-22.00
	+/- 2.69

	
	CMδe
	-2.02
	-11.15
	+/- 0.08

	IV
	CLα
	6.88
	7.89
	+/- 0.13

	
	CLq
	106.38
	57.99
	+/- 5.79

	
	CLδe
	0.99
	120.17
	+/- 0.18

	
	CMα
	-1.89
	-2.48
	+/- 0.06

	
	CMq
	-61.25
	-21.74
	+/- 2.70

	
	CMδe
	-2.01
	-10.74
	+/- 0.08

	V
	CLα
	8.66
	35.91
	+/- 0.43

	
	CLq
	134.32
	99.48
	+/- 13.64

	
	CLδe
	-0.69
	-254.78
	+/- 0.37

	
	CMα
	-2.39
	-29.44
	+/- 0.14

	
	CMq
	-69.15
	-37.46
	+/- 4.39

	
	CMδe
	-1.55
	14.51
	+/- 0.12

	VI
	CLα
	5.64
	-11.54
	+/- 0.03

	
	CLq
	5.90
	-91.24
	+/- 0.13

	
	CLδe
	0.08
	-82.23
	+/- 0.04

	
	CMα
	-1.71
	7.34
	+/- 0.01

	
	CMq
	-4.89
	90.28
	+/- 0.03

	
	CMδe
	-1.90
	-4.87
	+/- 0.01
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