7. Appendices

	Appendix 1:  Spec Sheet for Camera
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Appendix 2:  Spec Sheet for Heitronics
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Appendix 3:  Spec Sheet for Laser Altimeter
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Appendix X:  Piper Navajo

Basic Dimensions
Wing Span, ft (m) 					40.67 (12.39)
Wing Area, sq ft (sq m)				 	229 (21.3)
Length, ft (m) 						32.63 (9.946)
Height, ft (m) 						13.00 (3.962)
Wing Loading, lbs per sq ft (kg per sq m)		 	28.4 (139)
Power Loading, lbs per HP (kg per watt) 			10.5 (0.00639)
Propeller Diameter, in (m) 				80 (2.0)
Turning Radius (Nose Wheel), ft (m) 			28 (8.5)

Weights
Ramp Weight, lbs (kg) 					6,536 (2,965)
Gross Weight, Takeoff, lbs (kg)			 	6,500 (2,948)
Gross Weight, Landing Max				 6,200 (2,812)
Empty Weight (standard, six-place), lbs (kg) 		4,387 (1,990)
Useful Load (standard, six-place), lbs (kg) 			2,113 (958)

Power Plant
Engine Type Lycoming TIO-540-A
Rated Horsepower, HP (Watts) 				310 (231,167)
Rated Speed (rpm) 					2,575
Bore, inches (m) 						5.125 (0.1301)
Stroke, inches (m) 					4.375 (0.1111)
Displacement, cubic inches (cubic m) 			541.5 (0.008873)
Compression Ratio 					7.3:1
Dry Weight, lbs (kg) 					535.0 (242.67)
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